Appendix

♦Port numbers that NEC ESMPRO Manager uses
♦About services
♦Port numbers that NEC ESMPRO Manager uses

NEC ESMPRO Manager uses the following port numbers. In case of two-way protocol, upper arrow shows that connection starts, and lower arrow shows that connection turns. In case of port No. unknown, unused port is used to start connection. [ Web Client ←→Management PC ]
Function | Web Client | Protocol /direction | Management PC
Component | Port No. | Port No. | Component
Management/ monitoring | Web Browser | Unknown | TCP → ← | 8080 | NEC ESMPRO Manager

[ Management PC ←→Managed Server ]

Function | Management PC | Protocol /direction | Managed Server
Component | Port No. | Port No. | Component
Remote Console (CUI, non-SOL) | NEC ESMPRO Manager | 47115 | UDP → ← | 2069 | System BIOS
Remote Console (CUI, SOL) | NEC ESMPRO Manager | 47117(*1) | UDP → ← | 623 | BMC
Remote Console (GUI, GUI Remote Console Setting Enabled) | NEC ESMPRO Manager | Unknown | TCP → ← | 47130- 47139(*2) | NEC ESMPRO Agent Extension
Remote Console (GUI, GUI Remote Console Setting Disabled) | NEC ESMPRO Manager | Unknown | TCP → ← | 5900 | GUI Remote Console Function
Power Control | NEC ESMPRO Manager | 47117(*1) | UDP → ← | 623 | BMC
Remote Wake Up | NEC ESMPRO Manager | Unknown | UDP → | 10101 | LAN Card
Server Monitoring | NEC ESMPRO Manager | 47117(*1) | UDP → ← | 623 | BMC
Server Monitoring (SNMP) | NEC ESMPRO Manager | Unknown | UDP → ← | 161 | NEC ESMPRO Agent
Information Collection (through NEC ESMPRO Agent Extension) | NEC ESMPRO Manager | NEC ESMPRO Manager | TCP → ← | 47120- 47129(*2) | NEC ESMPRO Agent Extension
Information Collection (through BMC) | NEC ESMPRO Manager | 47117(*1) | UDP → ← | 623 | BMC
Remote Batch | NEC ESMPRO Manager | 47117(*1) | UDP → ← | 623 | BMC
Scheduled Running | NEC ESMPRO Manager | Unknown | TCP → ← | 47120- 47129(*2) | NEC ESMPRO Agent Extension
Operation with Command Line I/F | NEC ESMPRO Manager | 47117(*1) | UDP → ← | 623 | BMC
BMC configuration with network booting | NEC ESMPRO Manager PXE Service | 67 | UDP → ← | 68 | System BIOS
67 or 4011 | Unknown
69 | Unknown
Alert from BMC | NEC ESMPRO Manager | 162 | UDP ← | 623 | BMC
SNMP report to Manager | NEC ESMPRO Manager | 162 | UDP ← | Unknown | NEC ESMPRO Agent
TCP/IP report to Manager | NEC ESMPRO Manager | 31134 (*3) | TCP ← → | Unknown | NEC ESMPRO Agent
Search of Universal RAID Utility | NEC ESMPRO Manager | Unknown | UDP → ← | 427 | Universal RAID Utility
Universal RAID Utility | NEC ESMPRO Manager | Unknown | TCP → ← | Unknown | Universal RAID Utility
Universal RAID Utility event monitoring | NEC ESMPRO Manager | 8080 | TCP ← → | Unknown | Universal RAID Utility

*1 | The NEC ESMPRO Manager's port number used for communication with the BMC can be changed on the "Environment" screen.
*2 | The module uses the lowest unused port of the range.
*3 | The port number used by TCP/IP report to Manager can be changed in "TCP/IP Report Setting" screen of AlertViewer.

[ Management PC ←→ EM Card ]

Function | Management PC | Protocol /direction | EM Card
Component | Port No. | Port No. | Component
Information Collection | NEC ESMPRO Manager | 47117(*1) | UDP → ← | 623 | EM Card
NEC ESMPRO Manager | 47170-47179(*2) | TCP/IP ← | 623 | EM Card
NEC ESMPRO Manager | 47180-47189(*2) | UDP → ← | 623 | EM Card
Server Monitoring | NEC ESMPRO Manager | 47117(*1) | UDP → ← | 623 | EM Card
Server Monitoring (SNMP) | NEC ESMPRO Manager | Unknown | UDP → ← | 161 | EM Card
BMC configuration of CPU blade | NEC ESMPRO Manager | 47117(*1) | UDP → ← | 623 | EM Card
Operation with Command Line I/F | NEC ESMPRO Manager | 47117(*1) | UDP → ← | 623 | EM Card
SNMP Trap | NEC ESMPRO Manager | 162 | UDP ← | Unknown | EM Card
Ack sending for SNMP trap | NEC ESMPRO Manager | Unknown | UDP → | 5002 | EM Card

*1 | The NEC ESMPRO Manager uses a same port number for communication with BMC and EM card. The port number can be changed on the "Environment" screen.
*2 | The module uses the lowest unused port of the range.

[ Inside of the Management PC ]

Function | Component | Port No. | Protocol /direction | Port No. | Component
NEC ESMPRO Manager | NEC ESMPRO Manager | 1099 51099-51107(*1) | UDP → ← | 1099 51099-51107(*1) | NEC ESMPRO Manager
BMC Configuration with NEC ESMPRO Manager PXE Service | NEC ESMPRO Manager | Unknown | TCP → ← | 47160- 47169 | NEC ESMPRO Manager PXE Service
NEC ESMPRO Manager PXE Service | 31200 | UDP → ← | 31200 | NEC ESMPRO Manager PXE Service
NEC ESMPRO Manager Direct connection / Modem connection | NEC ESMPRO Manager | Unknown | TCP → ← | 47140- 47149(*1) | NEC ESMPRO Manager (DianaScope Modem Agent)

*1 | The module uses the lowest unused port of the range.

[ Management PC ←→ Other Vendor's Management Console ]

Function | Component | Port No. | Protocol /direction | Port No. | Component
SNMP Trap Redirection | NEC ESMPRO Manager | Unknown | UDP → | 162 | Other Vendor's Management Console

[About Applications run on the Management PC]

Function | Component | Port No. | Protocol /direction | Port No. | Component
Inter-Manager Communication | ESM Base Service | Unknown | TCP → ← | 8806 | ESM Base Service
Alert Viewer | Alert Viewer | Unknown | TCP → ← | 8807(*1) | ESM Alert Service

*1 | You can change the port number from [Tools] - [Port Settings] of AlertViewer.

♦About services

[NEC ESMPRO Manager]

NEC ESMPRO Manager uses the following services.
Service Name | Process Name | Function
Alert Manager Socket(R) Service | amvsckr.exe | Receiving TCP/IP In-bound report.(*1)
Dmi Event Watcher | dmieventwatcher.exe | Receiving DMI events.(*2)
ESM Alert Service | esmasvnt.exe | Receiving traps (alerts).
NVBASE System Service | nvbase.exe | Communication base for NEC ESMPRO Manager.
ESM Command Service | nvcmd.exe | Periodical command execution.
ESM Remote Map Service | nvrmapd.exe | Synchronizing Remote Map status color.
ESMPRO/SM Base Service | esmdsvnt.exe(*3) esmdsvap.exe | Server status watching.
ESMPRO/SM Trap Redirection | esmtrprd.exe | SNMP trap transferring function. (*2)
ESMPRO/SM Common Component | jsl.exe | Main service
ESMPRO/SM Web Container | jsl.exe | Web application server
DianaScope ModemAgent | DianaScopeModemAgent.exe | For modem/direct connection
*1 | This service has stopped when "Receive from Agent (TCP/IP)" of the TCP/IP Report Setting is disabled.
*2 | The startup is set as "Manual" by default.
*3 | For ESMPRO/SM Base Service, esmdsvnt.exe is registered as a service process, and esmdsvap.exe is started and stopped on starting and stopping the service.
♦ | About the dependencies of the services
| The dependencies of the services are the followings: NVBASE System Service ESM Alert Service Alert Manager Socket(R) Service Dmi Event Watcher ESM Command Service ESM Remote Map Service ESMPRO/SM Base Service ESMPRO/SM Trap Redirection ESMPRO/SM Common Component ESMPRO/SM Web Container DianaScope ModemAgent
♦ | About order of starting or stopping services
| To start or stop services, perform the following procedure. [Starting services] NVBASE System Service ESM Remote Map Service ESM Command Service ESM Alert Service Dmi Event Watcher(*) ESMPRO/SM Base Service ESMPRO/SM Trap Redirection(*) AlertManager Socket(R) Service(*) ESMPRO/SM Web Container ESMPRO/SM Common Component DianaScope ModemAgent [Stopping services] DianaScope ModemAgent ESMPRO/SM Common Component ESMPRO/SM Web Container AlertManager Socket(R) Service(*) ESMPRO/SM Trap Redirection(*) ESMPRO/SM Base Service Dmi Event Watcher(*) ESM Alert Service ESM Command Service ESM Remote Map Service NVBASE System Service
* | It may be stopped depending on the settings. In such a case, there is no need to start or stop the service.

[PXE Service]

The following services is installed when you select "PXE Service" on the installation.
Service Name | Process Name | Function
ESMPRO/SM PXE Agent Service | PxeAgent.exe | Command execution from the main service
ESMPRO/SM PXE TFTP Service | RMVtfldr.exe | A file transfer to the managed server
ESMPRO/SM PXE BINL Service | RMVBINLS.exe | The boot of the managed server
ESMPRO/SM PXE Main Service | RMVAUTH.exe | PXE Service main service
♦ | About procedures to start or stop services.
| To start or stop services, perform the following procedure with the services of NEC ESMPRO Manager started. [Start procedure] Start ESMPRO/SM PXE Agent Service from [Administrative Tools]-[Service]. After logging on NEC ESMPRO Manager, start the PXE Service from the Linkage Service of the header menu. (*) The following services start. ESMPRO/SM PXE TFTP Service ESMPRO/SM PXE BINL Service ESMPRO/SM PXE Main Service [Stop procedure] After logging on NEC ESMPRO Manager, stop the PXE Service form the Linkage Service of the header menu.(*) The following services stop. ESMPRO/SM PXE TFTP Service ESMPRO/SM PXE BINL Service ESMPRO/SM PXE Main Service Stop ESMPRO/SM PXE Agent Service from [Administrative Tools]-[Service].
* | If you start or stop the services from [Administrative Tools]-[Service], they do not function properly. They may have stopped according to the settings.