Settings after Installation

This page describes the necessary settings after the NEC ESMPRO Manager is installed. ♦ Manager
[Login]
When the installation of the NEC ESMPRO Manager completes, check that you can log in to it.
| 1. | Access to the following address on a Web browser on the Web client: http://"name of the server on which NEC ESMPRO Manager is installed":8080/esmpro/ The following example shows the address accessed from a Web browser on the NEC ESMPRO Manager server. http://localhost:8080/esmpro/
| The NEC ESMPRO Manager can be started up by clicking its icon created on the desktop after the installation.
| 2. | The NEC ESMPRO Manager login window opens. Enter the administrator name and the password that were registered at the installation, and click the [Login] button. When the login succeeds, the following window appears:
| The area on which commands, such as AlertViewer, Tools, and Search, are displayed is called "Header Menu". Use these commands on the "Header Menu" to operate the NEC ESMPRO Manager.
[Setting environment]
You can change the optional setting of the NEC ESMPRO Manager. Click "Environment Setting" on the "Header menu" to check the setting. For details, see the online help.
• | Set a modem The modem that is used to connect with a managed server should be set on the operating system on the NEC ESMPRO Manager server. If NEC ESMPRO Manager server has plural modem driver on Windows, input the modem name to use the connection in the DianaScopeModemAgent.ini file under the Sytem32 directory. The modem names are shown on device manager on Windows. The following is an example of DianaScopeModemAgent.ini file. modem=Standard 56000 bps modem
[SSL]
If you need to login to the NEC ESMPRO Manager using SSL, you should change the setting of the NEC ESMPRO Manager. Perform the procedure that is necessary in order to use SSL with the NEC ESMPRO Manager as follows:
1. | Create a key The Key tool is needed for creating the key using with SSL. The Key tool is contained in the JRE. Create the key as follows: In the case of NEC ESMPRO Manager installed in "C:\Program Files\ESMPRO": Windows(32 bits): "C:\Program Files\ESMPRO\ESMWEB\jre\bin\keytool" -genkey -alias tomcat -keyalg RSA Windows(64bits): "C:\Program Files (x86)\ESMPRO\ESMWEB\jre\bin\keytool" -genkey -alias tomcat -keyalg RSA Some messages are displayed with dialog style. Input the information about the creator of the key. You need to set the same password as the keystore password to the key password for <sdo>. The following is shown an example. Enter keystore password: ****** What is your first and last name? [Unknown]: Scott Oaks What is the name of your organizational unit? [Unknown]: SMCC What is the name of your organization? [Unknown]: Sun Microsystems What is the name of your City or Locality? [Unknown]: New York What is the name of your State or Province? [Unknown]: NY What is the two-letter country code for this unit? [Unknown]: US Is <CN=Scott Oaks, OU=SMCC, O=Sun Microsystems, L=New York, S=NY, C=US> correct? [no]: yes Enter key password for <sdo> (RETURN if same as keystore password): ****** Confirm that the key was created. Windows : %USERPROFILE%\.keystore
– | %USERPROFILE% means C:\Document and Settings\<logon user>
– | ~/means a home directory for logon user.
2. | Change the setting of NEC ESMPRO Manager Edit the server.xml file to enable SLL. The server.xml is in the directory ESMWEB\wbserver\conf on the NEC ESMPRO Manager installed directory. Open the server.xml file with an editor tool, search the description of <Connector> which is specified port number 8443, and delete the comment form "<!-" and "->". Modify the port number if you need. Add the keystore file path and the password that is specified at the time creating the keystore, in the description of <Connector>. <--Define a SSL HTTP/1.1 Connector on port 8443-->
<!-- NOTES: Delete these lines <Connector port="8443" NOTES: Change it if you need.
maxHttpHeaderSize="8192" maxThreads="150" minSpareThreads="25" maxSpareThreads="75" enableLookups="false" disableUploadTimeout="true" acceptCount="100" scheme="https" secure="true" clientAuth="false" sslProtocol="TLS"
keystoreFile="<the directory that contains keystore>/.keystore" keystorePass="<the password>" NOTES: Add these lines.
/>
--> NOTES:Add these lines.
3. | Reboot the NEC ESMPRO Manager server Reboot the server installed the NEC ESMPRO Manager.
4. | Login Confirm to login to the NEC ESMPRO Manager with "https:". Make access to the following address using the Web browser on the Web client.
| https://" the computer name installed the NEC ESMPRO Manager":" port number that is specified in server.xml"/esmpro/
An example of address to access from the web browser on the NEC ESMPRO Manager server is shown. https://localhost:8443/esmpro/
[Changing the port number]
You can change the available port number after installation of NEC ESMPRO Manager.
| 1. | Stop the following two services : - ESMPRO/SM Common Component - ESMPRO/SM Web Container
| 2. | Edit the port number in the "server.xml" setting file of ESMPRO/SM Web Container service. The "server.xml" file is on the "NEC ESMPRO Manager installed directory"\ESMWEB\wbserver\conf. In this file, you search the following <Connector> description specified port number 8080 and change the port number.
| 3. | Edit shortcut file "esmpro". The "esmpro" file is on the "NEC ESMPRO Manager installed directory"\ESMWEB. In this file, you search the following description specified port number 8080 and change the port number.
| 4. | Start the following two services. - ESMPRO/SM Common Component - ESMPRO/SM Web Container
[Coexistence with Tomcat] When NEC ESMPRO Manager and Tomcat are installed same computer, the application software installed later will not be running correctly. In this case, you can avoid it by the following way.
| 1. | If the following two services have started, stop the services. - ESMPRO/SM Common Component - ESMPRO/SM Web Container
| 2. | If Tomcat service has started, stop the service.
| 3. | Edit the port number in the "server.xml" setting file of ESMPRO/SM Web Container service. The "server.xml" file is on the "NEC ESMPRO Manager installed directory"\ESMWEB\wbserver\conf. In this file, you search the following description specified "Server port" number 8005 and change the port number to unused number.
| 4. | Start the following two services. - ESMPRO/SM Common Component - ESMPRO/SM Web Container
| 5. | Start Tomcat service.
– | Specify the port numbers of NEC ESMPRO Manager and Tomcat not to overlap. If you change the port number of NEC ESMPRO Manager, see the preceding clause "Change the Port Number".
– | When you use SSL communication on Tomcat or connect Tomcat with Apache, you may need to change another port number. See Tomcat's Document for detail.
[Update installation from an older version of NEC ESMPRO Manager]
If you perform update installation from the NEC ESMPRO Manager of less than version 5.0, the managed servers originally registered in the Operation Window will not be registered on the NEC ESMPRO Manager. To register the servers, perform auto-registration with this version of the NEC ESMPRO Manager.
– | When you perform update installation to the environment on which the NEC ESMPRO Manager under version 5.0 and the DianaScope Manager are installed, only the managed servers of the DianaScope Manager are registered until performing auto-registration.
– | Servers not to be monitored, such as Ver. 4.1 or prior version of NEC ESMPRO Agent, and maps are not registered.
– | The setting information that was set on NEC ESMPRO Manager Ver. 5.0 or prior will be inherited.