♦ NEC ESMPRO Manager PXE Service
[About installation]
• | NEC ESMPRO Manager PXE Service Installer cannot upgrade from NEC ESMPRO Manager PXE Service under Ver.1.01.01. Uninstall the older version, and then install new version. Note: All the registered information will be deleted as the result of the uninstalling.
• | NEC ESMPRO Manager PXE Service Installer cannot downgrade to the older version. If you want to use the older version, uninstall the current version and then install older version. Note: All the registered information will be deleted as the result of the uninstalling.
[About configuration] See 2.2.2.1 "Notes of Configuration with NEC ESMPRO Manager PXE Service" in "NEC ESMPRO Manager Ver.5 Setup Guide."
[Other PXE services and software with the PXE Service] Before starting the NEC ESMPRO Manager PXE Service, stop other PXE services and software having the PXE service function in the network. If you use other PXE services and software having the PXE service function, stop the NEC ESMPRO Manager PXE service and then start them. This procedure is necessary to start the service that you want to use. <How to stop/start NEC DeploymentManager that has PXE server function.> Click "Run" from [start] of Windows. Enter the command as following example. It shows case that the installed directory of NEC DeploymentManager is "C:\Program Files\NEC\DeploymentManager".
To stop the service | :
| "C:\Program Files\NEC\DeploymentManager\svcctrl" -stop
To start up the service | : | "C:\Program Files\NEC\DeploymentManager\svcctrl" -start

<How to stop/start Remote Install service>

To stop the service | : | Stop 3 services. Click [run] from [start] on Windows. Execute following each command: net stop BINLSVC net stop TFTPD net stop Groveler
To start up the service | : | Perform the following procedure:
1. | Click "control Panel" - "asministrative tool" - "Active Directory user and computer" from [start] on Windows.
2. | Find "Remote Install" server computer in the "Active Directory user and computer" snap in.
3. | Click the server computer and them click "Property".
4. | Click [Check server] on the "Remote install" tab.
5. | Follow the instruction of the wizard.

[About that the end of the network-boot procedure of
NEC ESMPRO Manager PXE Service]

Do not operate the destination server until network-boot procedure of NEC ESMPRO Manager PXE Service completes. When you have some operation before that, the NEC ESMPRO Manager PXE Service cannot be stopped from the NEC ESMPRO Manager.
For completion of the network boot, see 2.2.2.4 "How to confirm the status of the network-boot procedure by NEC ESMPRO Manager PXE Service" in "NEC ESMPRO Manager Ver.5 Setup Guide".

[About setting a Windows Firewall]

If the Windows Firewall is enabled on the management PC, NEC ESMPRO Manager PXE Service may not be executed BMC configuration.
In such a case, set the following ports on the management PC:
[Target ports]

Name (Can be changed) | Port number | Protocol
An arbitrary name | 67 | UDP
An arbitrary name | 69 | UDP
An arbitrary name | 4011 | UDP
An arbitrary name | 31200 | UDP