================================================================================
Express5800/R120h-1M
Express5800/R120h-1M (2nd-Gen)
Express5800/R120h-1M (3rd-Gen)
System ROM U32 v3.62 (01/09/2026)
================================================================================
Software name    : Express5800/R120h-1M, Express5800/R120h-1M (2nd-Gen),
                   Express5800/R120h-1M (3rd-Gen)
                   System ROM (BIOS) update module
Models           : Express5800/R120h-1M
                   Express5800/R120h-1M (2nd-Gen)
                   Express5800/R120h-1M (3rd-Gen)
Operating System : This software supports offline update and the following OS.
                   - Windows Server(R) 2012 R2
                   - Windows Server(R) 2016
                   - Windows Server(R) 2019
                   - Windows Server(R) 2022
                   - Windows Server(R) 2025
                   - Red Hat(R) Enterprise Linux(R) 7
                   - Red Hat(R) Enterprise Linux(R) 8
Target Users     : See [Target Users for Update] below
Type             : System ROM
================================================================================


[About the software]
The Express5800/R120h-1M, Express5800/R120h-1M (2nd-Gen),
Express5800/R120h-1M (3rd-Gen) System ROM (BIOS) update module supports
the following changes in the Express5800/R120h-1M,
Express5800/R120h-1M (2nd-Gen), Express5800/R120h-1M (3rd-Gen) models:

Upgrade Requirement: Critical - Update to this version immediately.

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - This version of the System ROM should be paired with Server Platform Services
   (SPS) Firmware 4.1.5.201 or later.

 - For systems installed with PMem (N8102-727, N8102-728, N8102-729) and a 
   system ROM version earlier than v2.90, please update the PMem firmware to
   version 1.2.0.5446 or later before updating to the system ROM version v3.10.
   If PMem is installed, the following information will be displayed on the 
   firmware screen (*1):

     HPE Persistent Memory [xx.xx.xx.xxxx] PROC [m] DIMM [n]
      [x]: Firmware version of HPE Persistent Memory
      [m]: Processor number
      [n]: DIMM number

     (*1) iLO Web Console > Firmware & OS Software > Firmware .

 Enhancements and problem fixes:
 - Addressed an issue where the system iLO Remote Console could become 
   unresponsive when a warning message appeared in RBSU.


  ** Program and data included in this software **
 Following program and data are included in this software.
 Use one of them according to the way of installation.
 After the update, the version will be: v3.62 (01/09/2026).

  a) ROM Flash Firmware Package
      \packages\OEM.U32_3.60_08_06_2025.fwpkg

  b) Executables for Windows(R)
      \packages\cp069597.exe

  c) RPM package for Linux(R)
      \packages\firmware-system-oem-u32-3.60_2025_08_06-1.1.x86_64.rpm

-------------------------------------------------------------------------------
[ Target Users for Update ]
This software is available for the users who use the following models with the
following System ROM version.

  - Models to be supported

     1. Express5800/R120h-1M
     2. Express5800/R120h-1M (2nd-Gen)
     3. Express5800/R120h-1M (3rd-Gen)

  - System ROM Versions to be supported

     1. U32 v1.00 (06/01/2017)
     2. U32 v1.20 (08/18/2017)
     3. U32 v1.22 (09/29/2017)
     4. U32 v1.26 (11/14/2017)
     5. U32 v1.32 (02/01/2018)
     6. U32 v1.36 (02/14/2018)
     7. U32 v1.42 (06/20/2018)
     8. U32 v1.46 (10/02/2018)
     9. U32 v2.00 (02/02/2019)
     10. U32 v2.02 (03/19/2019)
     11. U32 v2.04 (04/18/2019)
     12. U32 v2.10 (05/21/2019)
     13. U32 v2.16 (09/12/2019)
     14. U32 v2.22 (11/13/2019)
     15. U32 v2.30 (02/11/2020)
     16. U32 v2.32 (03/09/2020)
     17. U32 v2.34 (04/08/2020)
     18. U32 v2.36 (07/16/2020)
     19. U32 v2.42 (01/23/2021)
     20. U32 v2.54 (09/03/2021)
     21. U32 v2.58 (11/24/2021)
     22. U32 v2.62 (03/08/2022)
     23. U32 v2.66 (05/17/2022)
     24. U32 v2.68 (07/14/2022)
     25. U32 v2.80 (04/20/2023)
     26. U32 v2.90 (07/20/2023)
     27. U32 v3.10 (02/22/2024)
     28. U32 v3.34 (09/30/2024)

Note: In case of using newer System ROM from the above version, it has already
      applied equivalent enhancements. Updating the System ROM isn't needed.

Be sure to check the System ROM version and date with the following procedures.
Select an arbitrary procedure and check the version before and after the update.

 ** System Utilities **

 You can check the System ROM version and date by the following procedure.

    1. Power on the system and the contents of process by POST (Power On Self-
       Test) will be shown on the screen. After a short time, the following
       message is shown. Press <F9> key, "System Utilities" is started.

                        [F9] System Utilities

    2. After starting "System Utilities", select "System Information".

    3. Select "Firmware Information".

    4. Each firmware version is shown on the screen. The System ROM version and
       date can be seen at "System ROM" option.

  Note: After checking the System ROM version, press the <ESC> key or
        select "Exit" to exit the System Utilities.

  Note: About detail of "System Utilities" usage, refer to "1. System
        Utilities" section in the chapter of "Useful Features" of the
        maintenance guide.

 ** Windows(R) OS **

 You can check the System ROM date by a following procedure.

    1. Hold down <Windows> key and press <R> key.

    2. In the "Run" dialog box, type "msinfo32" and then click "OK".

    3. After "System Information" has started, select "System Summary".

    4. Check the System ROM version by the profile of "BIOS Version/Date".

 ** Linux(R) OS **

 You can check the System ROM date by a following procedure.

    1. Launch the terminal such as xterm.

    2. Execute the command as follows.

        # /usr/sbin/dmidecode | less

        Note: "#" means prompt. You do not need to input "#".

    3. Check the System ROM date by "BIOS Information->Release Date".

    Note: The dmidecode command has to be installed.

================================================================================
 Notes
================================================================================
  ** Notes in general **

  * Refer to "license_en.txt" about the user license agreement.

  * When you install the system ROM, the flashing mechanism writes over the
    backup ROM and saves current ROM as a backup, enabling you to switch easily
    to the alternate ROM version if the new ROM becomes corrupted for any
    reason. This feature protects the existing ROM version, even if you
    experience a power failure while flashing the ROM.

  * When Windows(R) BitLocker(TM) function is set to "Enabled", install the
    System ROM after making the function "Disabled". Then make the function
    "Enabled" after install and reboot of the system. If you install the system
    ROM without making the function "Disabled", you may need the recovery
    password when you boot the system.

  * This software does not support a virtualized environment such as hyper
    visor, guest OS, etc. Please install either on the OS which this software
    supports or with the method of offline installation.

  * To meet firmware dependencies, you can update iLO5 firmware by latest
    Starter Pack. And you can update Innovation Engine(IE) firmware by latest
    "Server Platform Services(SPS) firmware update module and Innovation
    Engine(IE) firmware update module".
    You can download latest update module(s) from the following web site.
    https://www.nec.com/express
    ("Support & Downloads" of the page top - PCs & Servers - Servers - Downloads
    - Select Model)

  * The system has System ROM version v2.00 or later and iLO5 firmware version
    1.38 or earlier when system temperature is low, fans may rotate at high
    speeds. This occurs because the iLO5 firmware version 1.38 or earlier does
    not support the temperature sensors for PMem that is defined in the System
    ROM v2.00 or later.

  ** Note for Windows(R) OS environment and Linux(R) OS environment **

  * This software will access to iLO5 (Baseboard Management Controller). It is
    required that the "iLO 5 Channel Interface Driver" (CHIF) must be installed.
    The CHIF driver can be installed by using EXPRESSBUILDER or "Starter Pack".

  ** Note for VMWare ESXi environment **

  * Do not update on a system that meets all the following conditions.
    OS :
      VMWare ESXi

    Processor :
     - Intel(R) Xeon(R) Bronze 31xx processor
     - Intel(R) Xeon(R) Silver 41xx processor
     - Intel(R) Xeon(R) Gold 51xx processor
     - Intel(R) Xeon(R) Gold 61xx processor
     - Intel(R) Xeon(R) Platinum 81xx processor

    BIOS/Platform Configuration(RBSU) :
     - Intel(R) TXT Support is set to Enabled.
          System Utilities > System Configuration >
          RBSU > Server Security >
          Intel(R) TXT Support

     - "Current TPM Type" of "Trusted Platform Module Options" is set to
       "TPM 1.2".
          System Utilities > System Configuration >
          RBSU > Server Security > Trusted Platform Module Options >
          Current TPM Type

        Note) The factory setting is "TPM 2.0".

--------------------------------------------------------------------------------
[Revision history]
Version:3.62 (01/09/2026)

Upgrade Requirement: Recommended 
                     - Update to this version at your earliest convenience.

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - This version of the System ROM should be paired with Server Platform Services
   (SPS) Firmware 4.1.5.201 or later.

 - For systems installed with PMem (N8102-727, N8102-728, N8102-729) and a 
   system ROM version earlier than v2.90, please update the PMem firmware to
   version 1.2.0.5446 or later before updating to the system ROM version v3.10.
   If PMem is installed, the following information will be displayed on the 
   firmware screen (*1):

     HPE Persistent Memory [xx.xx.xx.xxxx] PROC [m] DIMM [n]
      [x]: Firmware version of HPE Persistent Memory
      [m]: Processor number
      [n]: DIMM number

     (*1) iLO Web Console > Firmware & OS Software > Firmware .

 Enhancements and problem fixes:
 - Addressed an issue where the system iLO Remote Console could become 
   unresponsive when a warning message appeared in RBSU.

Version:3.60 (08/06/2025)

Upgrade Requirement: Recommended 
                     - Update to this version at your earliest convenience.

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - This version of the System ROM should be paired with Server Platform Services
   (SPS) Firmware 4.1.5.201 or later.

 - For systems installed with PMem (N8102-727, N8102-728, N8102-729) and a 
   system ROM version earlier than v2.90, please update the PMem firmware to
   version 1.2.0.5446 or later before updating to the system ROM version v3.10.
   If PMem is installed, the following information will be displayed on the 
   firmware screen (*1):

     HPE Persistent Memory [xx.xx.xx.xxxx] PROC [m] DIMM [n]
      [x]: Firmware version of HPE Persistent Memory
      [m]: Processor number
      [n]: DIMM number

     (*1) iLO Web Console > Firmware & OS Software > Firmware .

 Enhancements and problem fixes:
 - Addressed following security vulnerabilities.
    CVE-2025-20064, CVE-2025-20027, CVE-2025-20028, CVE-2025-20105

 - Updated microcode for Intel(R) Xeon(R) Scalable Processor family.

Version:3.50 (04/17/2025)

Upgrade Requirement: Recommended 
                     - Update to this version at your earliest convenience.

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - This version of the System ROM should be paired with Server Platform Services
   (SPS) Firmware 4.1.5.105 or later.

 - For systems installed with PMem (N8102-727, N8102-728, N8102-729) and a 
   system ROM version earlier than v2.90, please update the PMem firmware to
   version 1.2.0.5446 or later before updating to the system ROM version v3.10.
   If PMem is installed, the following information will be displayed on the 
   firmware screen (*1):

     HPE Persistent Memory [xx.xx.xx.xxxx] PROC [m] DIMM [n]
      [x]: Firmware version of HPE Persistent Memory
      [m]: Processor number
      [n]: DIMM number

     (*1) iLO Web Console > Firmware & OS Software > Firmware .

 Enhancements and problem fixes:
 - Updated microcode for Intel(R) Xeon(R) Scalable Processor family. This 
   version mitigates security vulnerability of CVE-2024-45332.

 - Removed Expired SUSE and Vmware Certificates.

 - Improved detection and interaction with certain PCIe cards during UEFI HBA 
   discovery process.

 - Addressed an issue where the system might trigger BitLocker Recovery after 
   reboot.

Version:3.42 (02/21/2025)

Upgrade Requirement: Critical - Update to this version immediately.

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - This version of the System ROM should be paired with Server Platform Services
   (SPS) Firmware 4.1.5.105 or later.

 - For systems installed with PMem (N8102-727, N8102-728, N8102-729) and a 
   system ROM version earlier than v2.90, please update the PMem firmware to
   version 1.2.0.5446 or later before updating to the system ROM version v3.10.
   If PMem is installed, the following information will be displayed on the 
   firmware screen (*1):

     HPE Persistent Memory [xx.xx.xx.xxxx] PROC [m] DIMM [n]
      [x]: Firmware version of HPE Persistent Memory
      [m]: Processor number
      [n]: DIMM number

     (*1) iLO Web Console > Firmware & OS Software > Firmware .

 Enhancements and problem fixes:
 - Added pop-up message for all Intelligent Provisioning boot paths to warn 
   users of the risk of data loss.

Version:3.40 (01/16/2025)

Upgrade Requirement: Recommended 
                     - Update to this version at your earliest convenience.

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - This version of the System ROM should be paired with Server Platform Services
   (SPS) Firmware 4.1.5.105 or later.

 - For systems installed with PMem (N8102-727, N8102-728, N8102-729) and a 
   system ROM version earlier than v2.90, please update the PMem firmware to
   version 1.2.0.5446 or later before updating to the system ROM version v3.10.
   If PMem is installed, the following information will be displayed on the 
   firmware screen (*1):

     HPE Persistent Memory [xx.xx.xx.xxxx] PROC [m] DIMM [n]
      [x]: Firmware version of HPE Persistent Memory
      [m]: Processor number
      [n]: DIMM number

     (*1) iLO Web Console > Firmware & OS Software > Firmware .

 Enhancements and problem fixes:
 - Updated microcode for Intel(R) Xeon(R) Scalable Processor family. This 
   version mitigates security vulnerability of CVE-2024-28956.

 - Addressed following security vulnerabilities.
    CVE-2024-28047

 - Addressed an issue where the system would uses UUID for IPV6 DHCP even when 
   the IPv6 DHCP Unique Identifier option(*2) is set to DUID-LLT.
    (*2) System Configuration > BIOS/Platform Configuration(RBSU)
         > Network Options > Network Boot Options
         > IPv6 DHCP Unique Identifier

 - Addressed an issue where the system uEFI Boot options might be de-selected 
   after updating the System ROM.

Version:3.34 (08/28/2024)

Upgrade Requirement: Optional - Update to this version at your convenience.

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - This version of the System ROM should be paired with Server Platform Services
   (SPS) Firmware 4.1.5.2.

 - If the system ROM version is v3.34 (09/30/2024), you cannot enable or disable
   new boot devices, nor can you save these settings in the UEFI Boot Order 
   Control menu(*1).
    (*1) BIOS/Platform Configuration (RBSU) > Boot Options 
         > UEFI Boot Order Control.

 - For systems installed with PMem (N8102-727, N8102-728, N8102-729) and a 
   system ROM version earlier than v2.90, please update the PMem firmware to
   version 1.2.0.5446 or later before updating to the system ROM version v3.10.
   If PMem is installed, the following information will be displayed on the 
   firmware screen (*2):

     HPE Persistent Memory [xx.xx.xx.xxxx] PROC [m] DIMM [n]
      [x]: Firmware version of HPE Persistent Memory
      [m]: Processor number
      [n]: DIMM number

     (*2) iLO Web Console > Firmware & OS Software > Firmware .

 Enhancements and problem fixes:
 - Addressed an issue where system may reboot infinitely when a faulty PCIe card
   was installed.

 - Addressed an issue where the firmware versions of iLO and Backplane showed
   incorrectly on System Utilities.

Version:3.32 (08/28/2024)

Upgrade Requirement: Recommended 
                     - Update to this version at your earliest convenience.

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - This version of the System ROM should be paired with Server Platform Services
   (SPS) Firmware 4.1.5.2.

 - For systems installed with PMem (N8102-727, N8102-728, N8102-729) and a 
   system ROM version earlier than v2.90, please update the PMem firmware to
   version 1.2.0.5446 or later before updating to the system ROM version v3.10.
   If PMem is installed, the following information will be displayed on the 
   firmware screen (*1):

     HPE Persistent Memory [xx.xx.xx.xxxx] PROC [m] DIMM [n]
      [x]: Firmware version of HPE Persistent Memory
      [m]: Processor number
      [n]: DIMM number

     (*1) iLO Web Console > Firmware & OS Software > Firmware .

 Enhancements and problem fixes:
 - Added support for Microsoft Windows Server 2025.

Version:3.30 (07/31/2024)

Upgrade Requirement: Recommended 
                     - Update to this version at your earliest convenience.

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - This version of the System ROM should be paired with Server Platform Services
   (SPS) Firmware 4.1.5.2.

 - For systems installed with PMem (N8102-727, N8102-728, N8102-729) and a 
   system ROM version earlier than v2.90, please update the PMem firmware to
   version 1.2.0.5446 or later before updating to the system ROM version v3.10.
   If PMem is installed, the following information will be displayed on the 
   firmware screen (*1):

     HPE Persistent Memory [xx.xx.xx.xxxx] PROC [m] DIMM [n]
      [x]: Firmware version of HPE Persistent Memory
      [m]: Processor number
      [n]: DIMM number

     (*1) iLO Web Console > Firmware & OS Software > Firmware .

 Enhancements and problem fixes:
 - Updated microcode for Intel(R) Xeon(R) Scalable Processor family.
   Addressed following security vulnerabilities.
    CVE-2024-24853

 - Addressed an issue where 480GB SSD Adapter for OS Boot (RAID 1)[N8103-239]
   may not be identified as an NVMe device.

 - Addressed an issue where the Logical Drive name was cleared in RBSU after
   leaving the configuration page of RAID Controller(N8103-240).

 - Addressed an issue where the "Physical Drive missing" message appeared twice
   in POST when a hard disk drive was removed and rebooted with incorrect
   severity in IML.

 - Addressed an issue where pressing the <F12> key and selecting [Save and Exit]
   in the UEFI Boot Order(*2) menu unexpectedly clears the boot order.
    (*2) System Configuration > BIOS/Platform Configuration(RBSU)
         > Boot Options > UEFI Boot Settings > UEFI Boot Order


Version:3.20 (05/27/2024)

Upgrade Requirement: Recommended 
                     - Update to this version at your earliest convenience.

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - This version of the System ROM should be paired with Server Platform Services
   (SPS) Firmware 4.1.5.2.

 - For systems installed with PMem (N8102-727, N8102-728, N8102-729) and a 
   system ROM version earlier than v2.90, please update the PMem firmware to
   version 1.2.0.5446 or later before updating to the system ROM version v3.10.
   If PMem is installed, the following information will be displayed on the 
   firmware screen (*1):

     HPE Persistent Memory [xx.xx.xx.xxxx] PROC [m] DIMM [n]
      [x]: Firmware version of HPE Persistent Memory
      [m]: Processor number
      [n]: DIMM number

     (*1) iLO Web Console > Firmware & OS Software > Firmware .

 Enhancements and problem fixes:
 - Addressed following security vulnerabilities.
    CVE-2021-38578, CVE-2023-5678, CVE-2024-0727

 - Added a new ""C6 without C1E"" parameter of Minimum Processor Idle Power Core
   C-State(*2) option to Power and Performance Options menu.
    (*2) System Configuration > BIOS/Platform Configuration(RBSU)
         > Power and Performance Options
         > Minimum Processor Idle Power Core C-State

Version:3.10 (02/22/2024)

Upgrade Requirement: Recommended 
                     - Update to this version at your earliest convenience.

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - This version of the System ROM should be paired with Server Platform Services
   (SPS) Firmware 4.1.5.2.

 - For systems installed with PMem (N8102-727, N8102-728, N8102-729) and a 
   system ROM version earlier than v2.90, please update the PMem firmware to
   version 1.2.0.5446 or later before updating to the system ROM version v3.10.
   If PMem is installed, the following information will be displayed on the 
   firmware screen (*1):

     HPE Persistent Memory [xx.xx.xx.xxxx] PROC [m] DIMM [n]
      [x]: Firmware version of HPE Persistent Memory
      [m]: Processor number
      [n]: DIMM number

     (*1) iLO Web Console > Firmware & OS Software > Firmware .

 Enhancements and problem fixes:
 - Addressed following security vulnerabilities.
    CVE-2021-38575, CVE-2023-45853

 - This version mitigates a security vulnerabilities (CVE-2022-36763, 
   CVE-2022-36764, CVE-2023-45229) in EDK2.

 - Prevented a non-standard VPD content from causing the UEFI read function to
   become write.

 - Added a new event support for IML.

 - Added an additional retry mechanisms to avoid a BIOS hang from iLO failure.

 - Addressed an issue where SBCE and ECC storm records may disappear from AHS.

 - Addressed an issue where the iSCSI SW IPv6 HDD could not be found under OS 
   when iSCSI IP Address Type option is set to Auto in BIOS/Platform 
   Configuration (RBSU) iSCSI Attempt Configuration menu.
         System Configuration > BIOS/Platform Configuration(RBSU) 
         > Network Options > iSCSI Configuration > Add an iSCSI Attempt 
         > iSCSI Network Interface Selection > iSCSI Attempt Configuration

 - Addressed an issue where the server may hang due to an IE function error.

 - Merged the solutions from EDK2 for vulnerabilities:
   - Buffer overflow in the DHCPv6 client via a long Server ID option
   - Out-of-bounds read when handling a ND Redirect message with truncated 
     options
   - Infinite loop when parsing unknown options in the Destination Options 
     header
   - Infinite loop when parsing a PadN option in the Destination Options header
   - Buffer overflow when processing DNS Servers option in a DHCPv6 Advertise 
     message
   - Predictable TCP ISNs
   - Use of a Weak PseudoRandom Number Generator

Version:3.00 (10/19/2023)

Upgrade Requirement: Recommended 
                     - Update to this version at your earliest convenience.

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - For systems that are installed with PMem (N8102-727, N8102-728, N8102-729), 
   please update the PMem firmware to version 1.2.0.5446 or later before 
   updating to system ROM v3.10.
   If PMem is installed, the following information will be displayed on the 
   firmware screen (*1):

     HPE Persistent Memory [xx.xx.xx.xxxx] PROC [m] DIMM [n]
      [x]: Firmware version of HPE Persistent Memory
      [m]: Processor number
      [n]: DIMM number

     (*1) iLO Web Console > Firmware & OS Software > Firmware .

 Enhancements and problem fixes:
 - Replaced AC power with external power in the help text of Automatic Power-On
   option.

 - Addressed an issue where BIOS did not report CPU status correctly to iLO when
   Uncorrectable Machine Check Exception (UMCE) occurs.

 - Addressed an issue where system might hang while accessing IML logs from
   RBSU.

Version:2.90 (07/20/2023)

Upgrade Requirement: Recommended 
                     - Update to this version at your earliest convenience.

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - For systems that are installed with PMem (N8102-727, N8102-728, N8102-729), 
   please update the PMem firmware to version 1.2.0.5446 or later before 
   updating to system ROM v2.90.
   If PMem is installed, the following information will be displayed on the 
   firmware screen (*1):

     HPE Persistent Memory [xx.xx.xx.xxxx] PROC [m] DIMM [n]
      [x]: Firmware version of HPE Persistent Memory
      [m]: Processor number
      [n]: DIMM number

     (*1) iLO Web Console > Firmware & OS Software > Firmware .

 Enhancements and problem fixes:
 - Updated microcode for Intel(R) Xeon(R) Scalable Processor family. 
   Addressed following security vulnerabilities.
    CVE-2022-43505, CVE-2022-40982

 - This version mitigates a security vulnerability (CVE-2023-2650) in OpenSSL.

 - Addressed an issue where iLO embedded device health info would display blank 
   content under System Utilities when the Select Language option was set to 
   Japanese or Chinese.

Version:2.80 (04/20/2023)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - When PMem(N8102-727, N8102-728, N8102-729) is installed and updated to
   System ROM v2.54 or later, PMem Firmware should be updated to
   version 1.2.0.5446 or later.

 Enhancements and problem fixes:
 - Added a new BIOS/Platform Configuration (RBSU) Omit Boot Device Event option
   to the Trusted Platform Module Options Menu.
         System Configuration > BIOS/Platform Configuration (RBSU)
         > Server Security > Trusted Platform Module Options
         > Omit Boot Device Event

 - Addressed following security vulnerabilities.
    CVE-2022-38087

 - Addressed the issue where the system might hang due to invalid memory free 
   and usage when TPM is enabled.

 - Addressed the issue where the TPM status between RBSU and iLO web pages was 
   not synchronized.

 - Addressed the issue where the power-on-password dialog popped up even though
   user did not set the password.

Version:2.76 (02/09/2023)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - When PMem(N8102-727, N8102-728, N8102-729) is installed and updated to
   System ROM v2.54 or later, PMem Firmware should be updated to
   version 1.2.0.5446 or later.

 Enhancements and problem fixes:
 - Added a new BIOS/Platform Configuration (RBSU) Energy Performance Preference 
   option to the Power and Performance Options Menu. 
         System Configuration > BIOS/Platform Configuration (RBSU)  
         > Power and Performance Options > UEFI Variable Access Firmware Control
         > Energy Performance Preference

 - Addressed following security vulnerabilities.
    CVE-2022-32231, CVE-2022-26343

 - This version mitigates a security vulnerability (CVE-2022-37434)
   in zlib library.

 - Addressed an issue where some Chinese and Japanese translations were missing 
   in RBSU.

 - Addressed an issue that system will hang when BIOS tries to print a large IML
   message on POST screen.

 - Addressed an issue when system discovers thousands of LUNs and was trying to 
   create thousands of boot options for each LUNs. System cannot add, delete or 
   adjust new boot options on iLO web and RBSU after rebooting. System becomes 
   unstable unless loading manufacture default.

Version:2.72 (09/29/2022)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - When PMem(N8102-727, N8102-728, N8102-729) is installed and updated to
   System ROM v2.54 or later, PMem Firmware should be updated to
   version 1.2.0.5446 or later.

 Enhancements and problem fixes:
 - Updated UEFI driver of PMem(N8102-727, N8102-728, N8102-729).

 - Added support to show manufacturing date for DIMMs in SMBIOS.

 - Improved the description of Memory Failed Events in the Integrated Management
   Log (IML).

 - Addressed an issue where a server running the ESXi hypervisor a with TPM 
   module installed would halt on loading modules after the installation of the 
   hypervisor OS, with the message "TPM log extend failed".

Version:2.68 (07/14/2022)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - When PMem(N8102-727, N8102-728, N8102-729) is installed and updated to
   System ROM v2.54 or later, PMem Firmware should be updated to
   version 1.2.0.5446 or later.

 Enhancements and problem fixes:
 - Updated microcode for Intel(R) Xeon(R) Scalable Processor family.
   Addressed an issue where the system may report UMCE to the Integrated
   Management Log (IML) with the following information when
   Intel(R) Hyper-Threading is set to Enabled.
       - Bank 0x3 or Bank 0x4
       - Status Code of 0xBE000000:00800400
 
 - This version mitigates a security vulnerability (CVE-2022-2068) in OpenSSL.

 - This version mitigates a security vulnerability (CVE-2022-27404,
   CVE-2022-27405, CVE-2022-27406) in FreeType library.

 - Addressed an issue where the system will hang with Red Screen of Death (RSOD)
   when user tries to switch Image Description option choices for NVMe devices
   under the Firmware Update menu in System Utilities.
         Embedded Applications > Firmware Update > [NVMe Device name]
         > Image Description

Version:2.66 (05/17/2022)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - When PMem(N8102-727, N8102-728, N8102-729) is installed and updated to
   System ROM v2.54 or later, PMem Firmware should be updated to
   version 1.2.0.5446 or later.

 Enhancements and problem fixes:
 - Added support for RAID Controller (4GB, RAID 0/1/5/6) [N8103-240].

 - This version mitigates a security vulnerability (CVE-2022-0778,
   CVE-2022-1292) in OpenSSL.

 - This version mitigates a security vulnerability (CVE-2019-7317)
   in libpng library.

 - This version mitigates security vulnerability of INTEL-SA-00601.

Version:2.64 (04/21/2022)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - When PMem(N8102-727, N8102-728, N8102-729) is installed and updated to
   System ROM v2.54 or later, PMem Firmware should be updated to
   version 1.2.0.5446 or later.

 Enhancements and problem fixes:
 - Updated microcode for Intel(R) Xeon(R) Scalable Processor family.
   This version mitigates security vulnerability of INTEL-SA-00616.

 - Updated hardware initialization code.

 - This version mitigates a security vulnerability (CVE-2018-25032)
   in zlib library.

 - Addressed an issue where RAID controller names were not displayed correctly
   in the PCIe Device Configuration menu in RBSU or the One-Time Boot menu
   when the Select Language option in System Utilities was set to non-English.
   But, when server was equipped with RAID Controller (4GB, RAID 0/1/5/6)
   [N8103-240], RAID controller name is not displayed correctly.
         System Configuration > BIOS/Platform Configuration (RBSU)
         > PCIe Device Configuration
 
 - Addresses an issue where the system would loop in reboot once the watchdog
   timer times out.

Version:2.62 (03/08/2022)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - When PMem(N8102-727, N8102-728, N8102-729) is installed and updated to
   System ROM v2.54 or later, PMem Firmware should be updated to
   version 1.2.0.5446 or later.

 Enhancements and problem fixes:
 - Addressed following security vulnerabilities.
   INTEL-SA-00527（CVE-2021-0099, CVE-2021-0103, CVE-2021-0107, CVE-2021-0111,
   CVE-2021-0114, CVE-2021-0115, CVE-2021-0116, CVE-2021-0117, CVE-2021-0118,
   CVE-2021-0125, CVE-2021-0124)

Version:2.60 (01/13/2022)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - When PMem(N8102-727, N8102-728, N8102-729) is installed and updated to
   System ROM v2.54 or later, PMem Firmware should be updated to
   version 1.2.0.5446 or later.

 Enhancements and problem fixes:
 - Addressed following security vulnerabilities.
   INTEL-SA-00527(CVE-2021-0092, CVE-2021-0093, CVE-2021-0144)

 - Addressed an issue where the systems with 480GB SSD Adapter for OS Boot
   (RAID 1)[N8103-239] may shut down intermittently and may log the following
   error message in the Integrated Management Log (IML).
   - System Overheating (Temperature Sensor 47, Location I/O Board,
     Temperature61) ACTION:Check fans, processor heat sink and air baffles
     installation.

 - Addressed an issue where the system may not automatically restart due to a
   hang condition during the POST when the IPMI Watchdog Timer option is
   enabled.
         System Configuration > BIOS/Platform Configuration (RBSU)  
         > System Options > Server Availability > IPMI Watchdog Timer

Version:2.58 (11/24/2021)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - When PMem(N8102-727, N8102-728, N8102-729) is installed and updated to
   System ROM v2.54 or later, PMem Firmware should be updated to
   version 1.2.0.5446 or later.

 Enhancements and problem fixes:
 - Added a new BIOS/Platform Configuration (RBSU) Platform Certificate Support
   option to the Server Security Menu.
   When TPM Visibility option is set to Hidden, Platform Certificate Support
   option must be set to Disabled.    
         System Configuration > BIOS/Platform Configuration(RBSU)
         > Server Security > Platform Certificate Support
    
         System Configuration > BIOS/Platform Configuration(RBSU) 
         > Server Security > Trusted Platform Module Options > TPM Visibility

 - Addressed an issue that can result in "Correctable Memory Error Threshold
   Exceeded" being logged to the Integrated Management Log (IML) incorrectly.

Version:2.56 (10/28/2021)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - When PMem(N8102-727, N8102-728, N8102-729) is installed and updated to
   System ROM v2.54 or later, PMem Firmware should be updated to
   version 1.2.0.5446 or later.

 Enhancements and problem fixes:
 - Updated microcode for Intel(R) Xeon(R) Scalable Processor family.
   This version mitigates security vulnerability of INTEL-SA-00532 for
   CVE-2021-0127 and INTEL-SA-0562 for CVE-2021-0157.

Version:2.54 (09/03/2021)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - When PMem(N8102-727, N8102-728, N8102-729) is installed and updated to
   System ROM v2.54 or later, PMem Firmware should be updated to
   version 1.2.0.5446 or later.

 Enhancements and problem fixes:
 - Addressed an issue where the following Uncorrectable Machine Check
   Exception and Uncorrectable Memory Errors may be reported and logged to
   the Integrated Management Log (IML) with certain DIMMs installed and
   the Extended Memory Test option is set to Enabled after updating
   the System ROM to v2.50 or v2.52. 
   - Uncorrectable Machine Check Exception (Processor X, APIC ID 0x000000xx,
     Bank 0x0000000x,...
   - DIMM Failure - Uncorrectable Memory Error (Processor X, DIMM Y)
     ACTION: Replace Failed DIMM.

   This issue does not impact systems configured Extended Memory Test in
   Disabled. The reported Uncorrected Memory Errors were due to an issue with
   the impacted System ROM revisions and do NOT indicate an issue with
   the DIMMs themselves.
         System Configuration > BIOS/Platform Configuration (RBSU)
         > System Options > Boot Time Optimizations > Extended Memory Test

Version:2.52 (07/08/2021)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 Enhancements and problem fixes:
 - Addressed following security vulnerabilities.
    CVE-2019-14584, CVE-2021-28211, CVE-2021-28210.

 - Addressed an issue where the memory channel numbering is incorrect for
   Correctable Memory Errors.

Version:2.50 (05/24/2021)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 Enhancements and problem fixes:
 - Added a new BIOS/Platform Configuration (RBSU) IPMI Watchdog Timer option
   to the Server Availability Menu. 
         System Configuration > BIOS/Platform Configuration (RBSU)  
         > System Options > Server Availability > IPMI Watchdog Timer

 - Added a new BIOS/Platform Configuration (RBSU) UEFI Variable Access Firmware
   Control option to the Server Security Menu. 
         System Configuration > BIOS/Platform Configuration (RBSU)  
         > Server Security > UEFI Variable Access Firmware Control

 - Updated the BIOS TPM 1.2 support for Windows Server 2022.

 - Updated the RESTful API BIOS Attribute Registry resources to match the
   latest BIOS/Platform Configuration(RBSU) options.

 - Addressed an issue where the system may experience an Unexpected Shutdown
   or a Bank 4 or a Bank 6 Machine Check with PMem(N8102-727, N8102-728,
   N8102-729) installed and configured for Memory Mode

 - Updated microcode for Intel(R) Xeon(R) Scalable processor family.
   Addressed following security vulnerabilities.
   INTEL-SA-00464

 - Updated hardware initialization code.
   Addressed following security vulnerabilities.
   INTEL-SA-00463

 - Addressed an issue where the server may become unresponsive during POST
   or take an unexpected long time to complete POST when the RBSU Extended
   Memory Test option was enabled.
         System Configuration > BIOS/Platform Configuration (RBSU)
         > System Options > Boot Time Optimizations > Extended Memory Test

 - Addressed an issue where the server was allowed to boot when mixed SKUs
   of Intel Xeon Scalable Processors are installed. 

 - Addressed an issue where the System ROM was logging a mismatched power supply
   condition with the latest version of the HPE Power Supplies. When this issue
   occurred, Dynamic Power Capping Functionality is set to Disabled and
   High Efficiency Mode in Redundant Power Supply Mode is set to Balanced Mode.
   To properly mitigate this issue, iLO Firmware version 2.50 or later is also
   needed.
         System Configuration > BIOS/Platform Configuration (RBSU) >
         System Options > Boot Time Optimizations
         > Dynamic Power Capping Functionality

         System Configuration > BIOS/Platform Configuration (RBSU) >
         Power and Performance Options > Advanced Power Options
         > Redundant Power Supply Mode

Version:2.42 (01/23/2021)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 Enhancements and problem fixes:
 - Updated the support for Fault Tolerant Memory (ADDDC) to improve system uptime.
         System Configuration > BIOS/Platform Configuration (RBSU) >
         Memory Options > Advanced Memory Protection
 
 - Updated microcode for Intel(R) Xeon(R) Scalable processor family.
   Addressed an issue where the system may report machine check exception(MCE)
   in the Integrated Management Log (IML) with the following information.
    - Bank 0x3 and MSCOD = 0080h and MCACOD = 0400h 
   or
    - Bank 0x9/0xA/0xB and MSCOD = 000Ch 

 - Added a new Posted Interrupt Throttle option to Advanced Performance Tuning
   Options menu. 
         System Configuration > BIOS/Platform Configuration (RBSU) >
         Power and Performance Options > Advanced Performance Tuning Options

 - Addressed an extremely rare issue where the Real Time Clock may become
   corrupted and an unexpected change on a server boot.

 - Addressed an issue where the Extended Memory Test is not run.
         System Configuration > BIOS/Platform Configuration (RBSU)
         > System Options > Boot Time Optimizations > Extended Memory Test

 - Addressed an issue where the server system fans may run higher than
   anticipated when a server is configured with SATA HDD/SSD (N8150-596,
   N8150-545, N8150-1734, etc.).
 
 - Addressed an issue where a bad LRDIMM memory device could be mapped out but
   was not properly reported in the Integrated Memory Log (IML). 

 - Added support to the BIOS/Platform Configuration (RBSU) Time Zones to
   add UTC-00:00 Dublin, London parameter. This support also requires
   the latest version of iLO 5 Firmware, version 2.40 or later.

Version:2.40 (10/26/2020)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 Enhancements and problem fixes:
 - Added a new Memory Options menu called Refresh Watermarks. 
   When selecting the Low Watermark setting, the memory controller will help
   reduce susceptibility to a DDR4 RowHammer attack. It is expected that
   a memory performance impact will be seen when enabling the Low Watermark
   setting.
         System Utilities > System Configuration > RBSU > Memory Options

 - Added support to DBX - Forbidden Signature Database to allow enrolling
   Secure Boot signature lists as a signed binary file. 
         System Utilities > System Configuration > RBSU > Server Security >
         Secure Boot Settings > Advanced Secure Boot options

 - Updated the System ROM to allow for an increased amount of 64-bit Memory
   Mapped I/O available for option cards. 

 - Updated the RESTful API BIOS Attribute Registry resources to match the
   latest BIOS/Platform Configuration(RBSU) options.

 - Updated hardware initialization code.
   This System ROM may improve memory stability.

 - Updated microcode for Intel(R) Xeon(R) Scalable processor family.

 - Addressed following security vulnerabilities.
   INTEL-SA-00381, INTEL-SA-00358, INTEL-SA-00390

 - Addressed an issue where the system may get stuck in a reboot loop during
   memory training. 

 - Addressed an issue where the memory locality of the ACPI SLIT table was not
   being created properly. 

 - Addressed an issue where the system would not properly call out a memory
   replacement event in the Integrated Management Log (IML) if
   Advanced Memory Protection option was configured to
   "Fault Tolerant Memory (ADDDC)" and an uncorrected memory failure occurred
   during an Advanced Double DRAM Device Correction (ADDDC) sparing operation.
         System Configuration > BIOS/Platform Configuration (RBSU) >
         Memory Options > Advanced Memory Protection

Version:2.36 (07/16/2020)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - When System ROM Version is v2.36 (07/16/2020), 
   Extended Memory Test option automatically becomes Disabled.
         System Configuration > BIOS/Platform Configuration (RBSU)
         > System Options > Boot Time Optimizations > Extended Memory Test

 Enhancements and problem fixes:
 - Updated to the latest thermal support for the platform.

 - Updated microcode for Intel(R) Xeon(R) Scalable processor family.

Version:2.34 (04/08/2020)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 Enhancements and problem fixes:
 - Updated to the latest thermal support for the platform.

 - Updated the RESTful API BIOS Attribute Registry resources to match the
   latest BIOS/Platform Configuration(RBSU) options.

 - Addressed an issue where the serial port would not function properly when
   the Serial CLI Status was also enabled on the server. This could lead to
   the serial BAUD rate not being configured properly and the serial output from
   the host would be corrupted or no output would be seen.
         System Configuration > BMC Configuration Utility > Setting Options
         > Serial CLI Status

 - Addressed an issue where UEFI Serial Debug output could inadvertently be seen
   over BIOS Serial Console when the BIOS Serial Console Port was enabled on
   the server. And, POST time will be increased about 2 minutes.
         System Configuration > RBSU > System Options > Serial Port Options
         > BIOS Serial Console and EMS > BIOS Serial Console Port

 - Addressed an extremely rare issue where the server could become unresponsive
   in POST when configured in Legacy BIOS Mode at Boot Mode option when a
   USB Mouse is attached. This issue does not impact systems configured 
   in UEFI Mode.
         System Configuration >  RBSU > Boot Options > Boot Mode

 - Addressed an issue where boot devices could disappear from the Boot Options
   menu when pressing the <F10> or <F12> key to save boot order changes.
         System Configuration >  RBSU > Boot Options

 - Addressed an issue where the system may report UMCE in the Integrated 
   Management Log (IML) with the following information.
    - Bank 0x9 or Bank 0xA or Bank 0xB
    - Status Code of 0xBE200000:000C110A

Version:2.32 (03/09/2020)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 - UEFI Serial Debug output could inadvertently be seen over BIOS Serial Console
   with System ROM v2.32 (03/09/2020). This issue would be seen periodically on
   server reboots. And, POST execution time will increase about 2 minutes.

 Enhancements and problem fixes:
 - Updated the UEFI driver of Smart Array S100i Software RAID.
   Addressed an issue where the Smart Array S100i Software RAID may experience
   potential data inconsistency during initial configuration or operation of
   a RAID volume configured in RAID 0/1/10.

Version:2.30 (02/11/2020)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 Enhancements and problem fixes:
 - Added a new "Balanced Performance Mode" parameter to "Persistent Memory
   Options > PMM Options > Performance Options" menu in BIOS/Platform
   Configuration(RBSU).

 - Added a new Persistent Memory NUMA Affinity Reporting menu to the Persistent
   Memory Options in the BIOS/Platform Configuration (RBSU). 

 - Updated to the latest thermal support for the platform.

 - Updated the RESTful API BIOS Attribute Registry resources to match the
   latest BIOS/Platform Configuration(RBSU) options.

 - Updated microcode for Intel(R) Xeon(R) Scalable processor family.
   Contents of update
    - This version mitigates security vulnerability of INTEL-SA-00329
      in Intel Corporation.
    - Addressed an issue where the system may report UMCE to the Integrated
      Management Log (IML) with the following information when Fast Fault
      Tolerant Memory Mode (ADDDC) is enabled.
       - Bank 0x7 or Bank 0x8
       - Status Code of 0xB2000000:00200400

 - Addressed an issue where the server may become unresponsive during POST when
   both iLO and the server are reset simultaneously.

 - Addressed an issue where the System Utilities System Information data could
   not be successfully exported to an FTP network location. 

Version:2.22 (11/13/2019)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 Enhancements and problem fixes:
 - Updated to the latest thermal support for the platform.

 - Updated the RESTful API BIOS Attribute Registry resources to match the
   latest BIOS/Platform Configuration(RBSU) options.

 - Addressed following security vulnerabilities.
    CVE-2017-5715, CVE-2019-0151, CVE-2019-0152, CVE-2019-11135, CVE-2019-11136,
    CVE-2019-11137, CVE-2019-11139

 - Updated microcode for Intel(R) Xeon(R) Scalable processor family.

 - Addressed an issue where the server may become unresponsive during POST
   when both iLO and the server are reset simultaneously.
    Note) The server stops POST by a message of "Memory Initialization Start".

 - Addressed an issue where the system may incorrectly report that a DIMM has
   been mapped out in the Integrated Management Log (IML) even though DIMM was
   not mapped out.

Version:2.16 (09/12/2019)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 Enhancements and problem fixes:
 - Updated microcode for Intel(R) Xeon(R) Scalable processor family.

Version:2.14 (09/05/2019)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 Enhancements and problem fixes:
 - Addressed an issue where the system may experience an uncorrectable memory
   error when 2nd Gen Intel(R) Xeon(R) Scalable processor family are installed
   with the following LRDIMM and Processor C-states are enabled.
   - 64GB DDR4-2933 LR Memory Kit (1x64GB/QR) [N8102-725]
   - 128GB DDR4-2933 LR Memory Kit (1x64GB/OR) [N8102-726]

Version:2.12 (07/03/2019)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 Enhancements and problem fixes:
 - Supported R120h-1M(3rd-Gen)[N8100-2834Y/2835Y].

Version:2.10 (05/21/2019)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 Enhancements and problem fixes:
 - Added a new BIOS/Platform Configuration (RBSU) IODC Configuration option to
   the Power and Performance Menu. 
         System Utilities > System Configuration >
         RBSU > Power and Performance Options > 
         Advanced Performance Tuning Options > IODC Configuration

   This option allows for tuning the policy for which I/O transactions interact
   with the processor cache.

 - Added support for Fast Fault Tolerant Memory (ADDDC) for memory configurations
   with single rank memory implemented. After updating the System ROM, the server
   will automatically configure Advanced Memory Protection option to Fault Tolerant 
   Memory (ADDDC) if both of the following two conditions are satisfied.
         System Utilities > System Configuration >
         RBSU > Memory Options > Advanced Memory Protection

    - A memory configuration that supports Fast Fault Tolerant Memory (ADDDC).
    - The configuration of Workload Profile is other than "Custom" and "Low latency".
         System Utilities > System Configuration >
         RBSU > Workload Profile

 - Addressed an issue where the Server Backup and Restore functionality may not
   work properly if initiated through the RESTful API returning a message "An
   internal error occurred during RIS operation".

 - Addressed an issue where the memory refresh rate is not set correctly when
   "Memory Refresh rate" option is "2x Refresh" parameter.
         System Utilities > System Configuration >
         RBSU > Memory Options > Memory Refresh Rate = 2x Refresh

   This issue was introduced with the v2.00 System ROM and did not impact
   earlier versions of the System ROM.

 - Addressed an issue where the system would not boot to a USB drive when a
   non-bootable (non-formatted) drive was also present in the system. This issue
   only impacts systems configured in Legacy BIOS Mode.
         System Utilities > System Configuration >
         RBSU > Boot Options > Boot Mode

 - Addressed following security vulnerabilities.
    CVE-2019-1559

Version:2.04 (04/18/2019)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 Enhancements and problem fixes:
 - Updated microcode for Intel(R) Xeon(R) Scalable Processor family.
   Contents of update
    - Addressed following security vulnerabilities.
       CVE-2018-12126, CVE-2018-12130, CVE-2018-12127, CVE-2019-11091,
       CVE-2019-0119, CVE-2019-0126
    - Addressed issues that may be cause for the following case.
       - Correctable or Uncorrectable Memory Errors
       - Uncorrectable Machine Check Exception (UMCE) Errors

 - Addressed an issue where the system boot time may be longer with the 
   following processors.
    - Intel(R) Xeon(R) Bronze 3xxx processor
    - Intel(R) Xeon(R) Silver 4xxx processor
    - Intel(R) Xeon(R) Gold 5xxx processor

Version:2.02 (03/19/2019)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 Enhancements and problem fixes:
 - Addressed following security vulnerabilities.
    CVE-2018-12201, CVE-2018-12202, CVE-2018-12203, CVE-2018-12204, 
    CVE-2018-12205

 - Updated microcode for Intel(R) Xeon(R) Scalable Processor family.

Version:2.00 (02/02/2019)

 Notes:
 - When using VMWare ESXi, be sure to refer to "** Note for VMWare ESXi
   environment **". PSOD(Purple Screen of Death) and system stop occurred after
   update of System ROM.

 Enhancements and problem fixes:
 - Added a new "Backup and Restore Settings" menu to "System Default Options" 
   in the BIOS/Platform Configuration (RBSU). This option allows you to save 
   the BIOS configuration to a USB storage device. 

 - Added a new "Dual Bifurcation" (quadfurcation) parameter of "PCIe Slot XX 
   Bifurcation option" to "Advanced PCIe Configuration Options" in BIOS/Platform
   Configuration(RBSU). This option will allow a x16 PCIe slot to be bifurcated 
   into four x4 PCIe slot. 

   Note) XX is PCIe Slot Number.
     This option is used for certain PCIe option cards that support/require
     PCIe slot bifurcation.

 - Updated description of Japanese and Chinese for System Utilities.

 - Updated the RESTful API BIOS Attribute Registry resources to match the
   latest BIOS/Platform Configuration(RBSU) options.

 - Addressed following security vulnerabilities.
    CVE-2018-3613, CVE-2017-5731, CVE-2017-5732, CVE-2017-5733, CVE-2017-5734, 
    CVE-2017-5735, CVE-2018-3630, CVE-2018-12178, CVE-2018-12179, 
    CVE-2018-12180, CVE-2018-12181, CVE-2018-12182, CVE-2018-12183

 - Updated microcode for Intel(R) Xeon(R) Scalable Processor family.

 - Addressed an issue where iLO virtual media may not boot properly after 
   setting the "Boot on Next Reset" option in the "Remote Console and Media - 
   Virtual Media" settings in the iLO web interface.

 - Addressed an issue where "Embedded Applications - Active Health System Log" 
   in System Utilities may fail to work properly with iLO5 firmware version
   1.30 or later.

 - Addressed an issue where an optional SATA DVD drive may not unlock and 
   allow media to be ejected after an operating system reboot.

 - Addressed an issue where the system may become unresponsive during boot and 
   experience a Red Screen (RSOD) when booting in Legacy BIOS Mode with a 
   M.2 SATA SSD installed. This issue does not impact systems in UEFI Mode.

 - Addressed an issue where difficult to input seconds part.
     System Utilities > System Configuration >
     RBSU > Date and Time > Time (hh:mm:ss)

 - Addressed an issue that lost setting information such as Serial Number and 
   Product ID recorded in the system if processing such as POST execution or 
   setting change is advanced while iLO is restarted.

 - Fixed the CPU L2 / L3 cache size display.
   System Utilities > System Information > Processor Information > L2 Cache
   System Utilities > System Information > Processor Information > L3 Cache

Version:1.50 (12/29/2018)

 Enhancements and problem fixes:
 - "Advanced Memory Protection" is now automatically changed to "Fast Fault 
   Tolerant Memory (ADDDC)" mode when the DIMM configuration supporting Fast 
   Fault Tolerant Memory Mode (ADDDC) and "Workload Profile" is other than "Low 
   Latency" and "Custom".

       System Utilities > System Configuration >
       RBSU > Processor Options > Workload Profile

       System Utilities > System Configuration >
       RBSU > Processor Options > Memory Options > Advanced Memory Protection

   Fast Fault Tolerant Memory (ADDDC) allows system to detect and correct errors
   before memory errors adversely affect the system, improving system fault 
   tolerance to memory problems.

   Note) When The following memory configuration is installed, "Fast Fault 
        Tolerant Memory Mode (ADDDC)" does not work. The "Advanced Memory 
        Protection" setting will remain.
        - A system that installs the following memory using x8 DRAM technology:
           8GB additional memory board(1x8GB/R/SR) [N8102-708]
           16GB additional memory board(1x16GB/R/DR) [N8102-710]
        - A system in which only one memory is installed in one memory channel.
           16GB additional memory board(1x16GB/R/SR) [N8102-709]

   Also, when "Advanced Memory Protection" is set to "Mirrored Memory with 
   Advanced ECC Support" mode or "Online Spare with Advanced ECC Support" mode, 
   the "Advanced Memory Protection" setting will remain.

   The automatic change to "Fast Fault Tolerant Memory (ADDDC)" mode can be 
   disabled by the following procedure.
   1. Press the <F9> key during POST to start up the system utility.
   2. Set "Workload Profile" to "Custom".
   3. Set "Advanced Memory Protection" to "Advanced ECC Support" mode.

Version:1.46 (10/02/2018)

 Firmware Dependencies:
 - To use the System ROM v1.46 (10/02/2018), following requirements should be
   met.

     1. iLO5 Firmware: Version 1.35 Aug 14 2018 or later
     2. Innovation Engine(IE) Firmware: Version 0.1.6.1 or later

   Note: About detail of update firmware(s), refer to "Notes in general" in
         this document.

 Enhancements and problem fixes:
 - Added support for flashing the firmware of the optional TPM (Trusted Platform
   Module) Kit. 

 - Added a new PCIe Peer-to-Peer Serialization option to the Advanced
   Performance Options menu in the BIOS/Platform Configuration (RBSU). 
   This option can be used to improve peer-to-peer performance between two
   PCIe devices installed on the same processor. 

 - Updated the RESTful API BIOS Attribute Registry resources to match the
   latest BIOS/Platform Configuration(RBSU) options.

 - Addressed an issue where early server video output, on a locally attached
   display, may not show correctly when the display is attached to the server
   through a KVM Switch.
   This issue does not impact video output on attached display that are not
   using a KVM Switch or video output through the iLO Integrated Remote Console.

 - Addressed an issue where firmware flashing through the RESTful API could
   periodically fail and the task being marked with an exception in the iLO
   Web interface. This issue could impact flashing firmware such as the
   Innovation Engine, Intel SPS Firmware or the TPM (Trusted Platform Module)
   Kit.

 - Addressed an issue where a PCIe option card would not properly train to its
   maximum speed when the PCIe Bifurcation option was enabled. This issue does
   not impact PCIe option cards that do not require bifurcation.

 - Addressed an extremely rare issue where a system configured with a SATA DVD
   drive and a Smart Array controller may become unresponsive during boot,
   usually with a Red Screen of Death (RSOD), when in legacy BIOS mode. This
   issue does not impact systems configured in UEFI Mode.

 - Addressed an issue where a PCIe option card's legacy option ROM may not
   properly display its legacy setup menu prompt during boot when in legacy
   BIOS mode. This issue does not impact systems configured in UEFI Mode.

Version:1.42 (06/20/2018)

 Firmware Dependencies:
 - To use the System ROM v1.42 (06/20/2018), following requirements should be
   met.

     1. iLO5 Firmware: Version 1.35 Aug 14 2018 or later
     2. Innovation Engine(IE) Firmware: Version 0.1.6.1 or later

   Note: About detail of update firmware(s), refer to "Notes in general" in
         this document.

 Enhancements and problem fixes:
 - Updated microcode for Intel(R) Xeon(R) Scalable Processor family.
   This version mitigates security vulnerability of INTEL-SA-00115 and INTEL-
   SA-00161 in Intel Corporation.

 - Addressed an issue where systems may experience an 389 - Unexpected Shutdown
   and Restart - An undetermined error type resulted in a reboot of the server,
   logged in the iLO Integrated Management Log (IML).

 - Addressed an issue where systems may log an erroneous Bank 4 Machine Check
   Exception (MCE) to the IML on a system reset event. 

Version:1.40 (06/15/2018)

 Firmware Dependencies:
 - To use the System ROM v1.40 (06/15/2018), the following requirements
   should be met.

     1. iLO5 Firmware: Version 1.30 May 31 2018 or later
     2. Innovation Engine(IE) Firmware: Version 0.1.6.1 or later

   If the requirements aren't met, update to the appropriate firmware(s).

 Enhancements and problem fixes:
 - Added support for the latest VMware vSphere Secure Boot Certificate.
   When you intend to use this new certificate, you need to reset "Allowed
   Signatures Database" by selecting "Reset to Platform default" in
   System Utilities. And then you need to reconfigure Secure Boot settings.

 - Added support to decode certain Machine Check Exceptions(MCE) to a specific
   failing PCIe device. Previous versions of the System ROM would log a generic
   MCE to the Integrated Management Log (IML) for these error events.

 - Added a new "Memory Controller Interleaving" to "Memory Options" option of
   BIOS/Platform Configuration(RBSU). This option allows disabling memory
   controller interleaving which may improve memory performance for systems
   configured with an unbalanced memory configuration.

 - Added a new "Processor Jitter Control Optimization" to "Advanced Performance
   Options" option of BIOS/Platform Configuration(RBSU). This option setting
   allows users to choose between optimizing Auto-tuned mode for maximum
   throughput performance, low latency, or the default - zero latency.

 - Updated the RESTful API BIOS Attribute Registry resources to match the
   latest BIOS/Platform Configuration(RBSU) options.

 - Updated description of Japanese and Chinese for System Utilities.

 - Addressed an issue where the IML Viewer in the System Utilities menu may
   become unresponsive when launched.

 - Addressed an issue where the Dual microSD Card USB Module may not boot
   properly when the UEFI POST Discovery Mode option is set to Force Fast
   Discovery.

 - Addressed an issue where the Trusted Platform Module (TPM) Firmware update
   may not complete properly when the TPM is configured for "TPM 2.0" Mode.
   This issue does not impact systems configured with a TPM operating in
   "TPM 1.2" mode.

 - Addressed an issue where the system may not be able to boot to EXPRESSBUILDER
   when a specific USB Key was installed in one of the server USB Ports.

 - Addressed an issue where iLO Virtual Media may not boot properly when the
   "UEFI POST Discovery Mode" option is set to "Force Full Discovery".

 - Addressed an issue where the system may become unresponsive during POST or
   experience a Red Screen on the next boot following an I/O Machine Check
   Exception (MCE) at runtime.

 - Addressed an issue where a system configured with the "Internal SD Card"
   disabled from BIOS/Platform Configuration (RBSU) and an Dual microSD card
   installed would not boot from the Dual microSD card USB Module when
   configured in "Legacy Boot Mode". This issue does not impact systems
   configured in UEFI Boot Mode.

 - Addressed an issue where systems configured with Smart Array S100i SR Gen10
   may experience a failed RAID volume on a system reset.

Version:1.36 (02/14/2018)

 Enhancements and problem fixes:
 - Added new "Storage Device Information" to "System Information" menu of
   System Utilities.
 
 - Added new "PCIe Bifurcation Options" menu and "PCIe Slot XX Bifurcation"
   options to BIOS/Platform Configuration(RBSU). (XX is PCIe Slot Number.)
   When enabled, this option will bifurcate a PCIe slot into two equal width
   slots. This option is used for certain PCIe option cards that 
   support/require PCIe slot bifurcation. 

 - Added a new "Direct to UPI(D2K)" option to "Power and Performance Options"
   of BIOS/Platform Configuration(RBSU). If the default "Auto" parameter is
   selected, the function is configured to "Enabled" or "Disabled"
   appropriately. Use this option in "Auto" of default unless otherwise
   specified.

 - Added a new "Enhanced CPU Cooling" parameter to "Thermal Configuration"
   option of "Fan and Thermal Options" in BIOS/Platform Configuration(RBSU).
   When running certain processor intensive workloads, this option can
   provide additional cooling to the processors which can result in improved
   performance. 

 - Added support for wheel functionality of the iLO virtual mouse in the System
   Utilities. In Addition, the wheel function of the virtual mouse is supported
   with iLO5 firmware version 1.20 or later.
   
 - Added RESTful API configuration support for the Smart Array S100i SR Gen10 SW
   RAID controller.
 
 - Updated the RESTful API BIOS Attribute Registry resources to match the
   latest BIOS/Platform Configuration(RBSU) options.

 - Updated description of Japanese and Chinese for System Utilities.

 - Addressed an issue where the UEFI Boot Order would not get reset to a default
   value when loading a default configuration. This issue does not impact
   systems configured in Legacy Boot Mode. 

 - Addressed an issue where the High Performance Event Timer (HPET) was
   reported as "not functioning properly" under Device Manager on Windows(R).

 - Addressed an issue where the "Embedded Serial Port" option could not be
   properly configured through the RESTful Interface.

 - Addressed an issue where the PCI Express I/O Proximity values were not
   properly allocated in the ACPI System Locality Information Table (SLIT).
   This change may help provide a performance benefit in applications and
   configurations that are sensitive to PCIe Device I/O NUMA awareness.

 - Addressed a rare issue where the system may become unresponsive when a SAS
   drive was inserted with the Smart Array S100i SR Gen10 SW RAID enabled.
   This issue does not impact systems configured in AHCI mode.

 - Addressed an issue where the system may experience an erroneous boot-time
   message and Integrated Management Log (IML) entry stating that Core Boost
   Technology is disabled due to a lack of an iLO Advanced License (531 -
   Core Boost Technology missing required iLO License).

Version:1.32 (02/01/2018)

 Enhancements and problem fixes:
 - Updated microcode for Intel(R) Xeon(R) Scalable Processor family.
   This version mitigates security vulnerability of INTEL-SA-00088 in Intel
   Corporation.

 - Addressed an issue where the system may experience an erroneous boot-time
   message and Integrated Management Log (IML) entry stating that Core Boost
   Technology is disabled due to a lack of an iLO Advanced License (531 -
   Core Boost Technology missing required iLO License).

Version:1.26 (11/14/2017)

 Enhancements and problem fixes:
 - Added support for update function of Innovation Engine (IE) Firmware revision
   0.1.4.4 and later. 
   Updating System ROM to v1.26 is needed to apply IE Firmware 0.1.4.4 and SPS
   Firmware 4.0.4.288 or later. These version of firmware mitigate security
   vulnerability of INTEL-SA-00086 in Intel Corporation.
   
 - Addressed an issue where the High Performance Event Timer (HPET) was
   reported as "not functioning properly" under Device Manager on Windows(R).

Version:1.22 (09/29/2017)

 Enhancements and problem fixes:
 - Addressed an issue where the system would not achieve maximum performance
   results when the BIOS/Platform Configuration (RBSU) Sub-NUMA Clustering
   option is enabled. This option is not enabled by default.

 - Addressed an issue where the system may have the system time incorrectly
   "shifted" to the incorrect time after the operating system has been running
   for an extended period of time. This issue was typically seen under
   Microsoft Windows(R) when the Set Time Automatically option was enabled from
   the Windows Date and Time Settings configuration page.

 - Addressed an issue where the system may report an inaccurate error message
   in the Integrated Management Log (IML) when a memory training failure
   occurred. It is recommended that customers update to this version of the
   system ROM before replacing any DIMMs due to a training issue.

 - Addressed an issue where the system may experience an erroneous boot-time
   message and Integrated Management Log (IML) entry stating that Core Boost
   Technology is disabled due to a lack of an iLO Advanced License (531 - Core
   Boost Technology missing required iLO License) when using the Version 1.20
   System ROM.

Version:1.20 (08/18/2017)

 Enhancements and problem fixes:
 - Added support for Dynamic Power Capping. This feature can be enabled from
   the BIOS/Platform Configuration (RBSU) Boot Time Optimizations Menu.
   This support requires Power Management Controller Firmware version 1.0.4
   and iLO5 Firmware version 1.15 or later.

 - Added support for the Core Boost Technology. This feature requires
   IE Firmware 0.1.2.6 or later.

 - Added a new BIOS/Platform Configuration (RBSU) Power and Performance Tuning
   option for LLC Dead Line Allocation. When running certain applications,
   modifying this setting from its default value may improve system performance.

 - Added a new BIOS/Platform Configuration (RBSU) Power and Performance Tuning
   option for Stale A to S. When running certain applications, modifying this
   setting from its default value may improve system performance.

 - Added support to detect and report unbalanced memory configurations that may
   result in non-optimal performance. Please consult the User's Guide for more
   information on memory population rules and recommendations.

 - Added a new Auto option for the XPT Prefetcher in the BIOS/Platform
   Configuration (RBSU) menu that will default the XPT Prefetcher to disabled
   based on a current Intel sighting processor issue.  Enabling this option
   (via setting this option for Force Enable) may improve latency performance,
   but Intel has indicated rare stability issues may occur if XPT Prefetcher
   is enabled.

 - Added support for 128GB Load Reduced DIMMs (LRDIMMs).

 - Updated the system thermal logic to support the latest GPU adapters.

 - Updated the RESTful API BIOS Attribute Registry resources to match the
   latest BIOS/Platform Configuration options.

 - Updated the language translations (non-English modes) for System Utilities.

 - Added support for "Fast Fault Tolerant (ADDC)" option on Advanced Memory
   Protection.

 - Addressed an issue where the UEFI or Legacy Boot Order could still be
   modified after an incorrect Administrator Password was entered in the
   BIOS/Platform Configuration (RBSU) menus.

 - Addressed an issue where the embedded AHCI SATA controller would not
   show up properly in the BIOS/Platform Configuration (RBSU) PCI Devices
   menu when no drives were attached to the controller.

 - Addressed an issue where saving a configuration setting from an optional
   device's configuration page in the System Utilities menu would not be
   saved properly.  This issue was seen with one Network Adapter card.

 - Addressed an issue where the system ROM would not correctly report 
   a configuration error for the Smart Battery storage subsystem when more
   devices were installed than could be supported by the installed battery.

 - Addressed an issue where a platform configured with direct attached NVMe
   hard drives may report the incorrect location (box and bay location) from
   the System Utilities page.

 - Addressed an issue where the System Utilities menu may not show the proper
   name for an optional PCIe Adapter.

 - Addressed an issue where the chassis power supply information would not be
   properly reported from the Industry Standard SMBIOS records.

 - Addressed an issue where the iLO remote Console Keyboard and Mouse may not
   function properly when the system is configured for Legacy Boot Mode. This
   issue does not exist on systems configured in UEFI Boot Mode.

 - Addressed an issue where the Jitter Performance feature settings could not
   be properly modified from the iLO web interface.

 - Addressed an issue where the system may report that the Smart Battery is
   charging when in fact the battery has failed. It is recommended to flash
   to this system ROM if a system is reporting Smart Battery issues.

 - Addressed an issue where the Trusted Platform Module (TPM) option for TPM
   Visibility could not be configured through the RESTful API.

 - Addressed an issue where the system may become unresponsive when repeatedly
   typing characters, such as DIR, in Legacy Boot Mode from a pre-OS
   environment. This issue does not impact systems in UEFI Boot Mode or
   a system once the system boots into an operating system.

 - Addressed an issue where certain third party PCIe adapters, such as
   a Dialogic adapter, would not function properly due to the PCIe Maximum
   Payload size being incorrectly programmed.

 - Addressed an issue where certain NVMe devices may not be detected when the
   x16 slot PCIe Riser and three slot x8 riser are present in the server.

 - Addressed an issue where a Network Boot option would still show an entry
   in the Legacy Boot Order when Network Boot was disabled on the device from
   the BIOS/Platform Configuration (RBSU) Network Options Menu. This issue does
   not affect systems configured for UEFI Boot Mode.

 - Addressed an issue where the system may become unresponsive when using the
   TAB key in the BIOS/Platform Configuration (RBSU) menus.

 - Addressed an issue where the BIOS would not properly identify and halt
   a system from booting with an invalid DIMM configuration.

 - Addressed an issue where the BIOS/Platform Configuration (RBSU) Energy
   Efficient Turbo setting was "backwards".  When the configuration setting
   was set to enabled, the feature would actually be Disabled. When configured
   to Disabled, the feature would actually be enabled.

 - Addressed an issue where the server might lockup and display a red screen
   when trying to repair a failed RAID volume off of an S100i SW RAID
   controller.

 - Addressed an issue where the RESTful API may report that BIOS settings were
   not applied properly even when they are properly configured.

 - Addressed an issue where the system may become unresponsive during boot after
   a warm reset, typically seen with a blank screen, when a Trusted Platform
   Module (TPM) is installed. If reboot issues are seen with systems containing
   an optional TPM, it is highly recommended the System ROM be enabled to this
   revision or later.

 - Addressed an extremely rare issue where the system may incorrectly report
   a 413 Innovation Engine Authentication Error on a server reboot.

 - Removed support for the BIOS/Platform Configuration (RBSU) Power On Logo
   disable functionality.

 - Removed the Platform Configuration (RBSU) Option to enable or disable the
   Embedded Diagnostics. Embedded Diagnostics is not supported on this server
   and the menu option should not have been available and was not functional.

 - Remove Embedded Diagnostics support from System Utilities.

 - Removed support for the chipset firmware based Trusted Platform Module (TPM)
   known as Intel Platform Trust Technology (Intel PTT). This feature is no
   longer supported due to stability issues and Intel recommends not supporting
   this feature. Users should instead install a TPM kit for this support.

 - Addressed an issue the "iLO LUN 00 Media 0 USB Device" always exists.

--------------------------------------------------------------------------------
[Copyright and Trademark]

All contents on this software are the copyright of NEC Corporation or the
third-party software developer. All other contents mentioned herein are
copyright of their respective owners.

Microsoft, Windows, Windows Server are trademarks or registered trademarks of
Microsoft Corporation in the United States and other countries.
Linux(R) is a registered trademark of Linus Torvalds in the United States and
other countries.
Red Hat is a trademark or a registered trademark of Red Hat Inc. in the United
States and other countries.

All other company names and product names mentioned herein are registered
trademarks or trademarks of their respective owners.

--------------------------------------------------------------------------------
   Copyright NEC Corporation 2026
