===============================================================================
1. Preparing the iLO5 binary file
===============================================================================
(1) Download Starter Pack Version S8.10-010.11
    https://www.58support.nec.co.jp/global/download/index.html
    - select your server model
    - Download E8.10-010.011
(2) Extract the iLO5 pakage file
    Extract the following file from the "packages" folder of the downloaded
    ISO file using a decompression tool such as 7-Zip:
    - ilo5_309.fwpkg
(3) Extract the iLO5 binary file
    Extract the following file from the extraced iLO5 pakage file a using a
    decompression tool such as 7-Zip:
    - ilo5_310.bin

===============================================================================
2. Updating the iLO5 Firmware
===============================================================================
Update the iLO5 firmware.
(1) Login to the iLO Web Interface.
(2) Navigate to [Firmware & OS Software] - [Update Firmware].
(3) The "Flash Firmware" page will be displayed. Select "Local file" for "File
    location", then click the "Browse" button for "Local binary file" and
    select "ilo5_310.bin".
    Do not check [Also store in iLO Repository] or [Update Recovery Set].
(4) Click the "Flash" button to perform the update.
    If a confirmation message appears, select "OK" to proceed.
(5) After the firmware update completion message, an iLO reset will occur,
    and the connection with the browser will be terminated.
(6) Please close your web browser temporarily.
    Once login becomes possible, access the iLO Web Interface URL again, and
    reconnect by entering your login/password.
(7) Navigate to [Firmware & OS Software] - [Firmware].
(8) Verify if the iLO5 firmware version is "3.10 Dec 12 2024".
