================================================================================
Express5800/R110j-1
System ROM U43 v3.72 (01/09/2026)
================================================================================
Software name    : Express5800/R110j-1
                   System ROM (BIOS) update module
Models           : Express5800/R110j-1
Operating System : This software supports offline update and the following OS.
                   - Windows Server(R) 2012 R2
                   - Windows Server(R) 2016
                   - Windows Server(R) 2019
                   - Windows Server(R) 2022
                   - Red Hat(R) Enterprise Linux(R) 7
                   - Red Hat(R) Enterprise Linux(R) 8
Target Users     : See [Target Users for Update] below
Type             : System ROM
================================================================================


[About the software]
The Express5800/R110j-1 System ROM (BIOS) update module supports the following
changes in the Express5800/R110j-1 models:

Upgrade Requirement: Critical - Update to this version immediately.

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - This version of the System ROM should be paired with Server Platform Services
   (SPS) Firmware 5.1.5.103 or later.

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Addressed an issue where the system iLO Remote Console could become 
   unresponsive when a warning message appeared in RBSU.


  ** Program and data included in this software **
 Following program and data are included in this software.
 Use one of them according to the way of installation.
 After the update, the version will be: v3.62 (01/09/2026).

  a) ROM Flash Firmware Package
      \packages\OEM.U43_3.70_08_08_2025.fwpkg

  b) Executables for Windows(R)
      \packages\cp069616.exe

  c) RPM package for Linux(R)
      \packages\firmware-system-oem-u43-3.70_2025_08_08-1.1.x86_64.rpm

-------------------------------------------------------------------------------
[ Target Users for Update ]
This software is available for the users who use the following models with the
following System ROM version.

  - Models to be supported

     1. Express5800/R110j-1

  - System ROM Versions to be supported

     1. U43 v1.02 (10/02/2018)
     2. U43 v1.03 (11/28/2018)
     3. U43 v1.20 (02/02/2019)
     4. U43 v1.22 (04/04/2019)
     5. U43 v2.00 (05/16/2019)
     6. U43 v2.10 (09/12/2019)
     7. U43 v2.12 (12/06/2019)
     8. U43 v2.14 (03/09/2020)
     9. U43 v2.16 (05/25/2020)
     10. U43 v2.18 (06/24/2020)
     11. U43 v2.20 (10/27/2020)
     12. U43 v2.23 (02/19/2021)
     13. U43 v2.32 (06/10/2021)
     14. U43 v2.52 (09/16/2021)
     15. U43 v2.54 (10/21/2021)
     16. U43 v2.56 (01/20/2022)
     17. U43 v2.60 (07/14/2022)
     18. U43 v2.68 (01/12/2023)
     19. U43 v2.80 (07/20/2023)
     20. U43 v3.10 (05/16/2024)
     21. U43 v3.40 (08/01/2024)

Note: In case of using newer System ROM from the above version, it has already
      applied equivalent enhancements. Updating the System ROM isn't needed.

Be sure to check the System ROM version and date with the following procedures.
Select an arbitrary procedure and check the version before and after the update.

 ** System Utilities **

 You can check the System ROM version and date by the following procedure.

    1. Power on the system and the contents of process by POST (Power On Self-
       Test) will be shown on the screen. After a short time, the following
       message is shown. Press <F9> key, "System Utilities" is started.

                        [F9] System Utilities

    2. After starting "System Utilities", select "System Information".

    3. Select "Firmware Information".

    4. Each firmware version is shown on the screen. The System ROM version and
       date can be seen at "System ROM" option.

  Note: After checking the System ROM version, press the <ESC> key or
        select "Exit" to exit the System Utilities.

  Note: About detail of "System Utilities" usage, refer to "1. System
        Utilities" section in the chapter of "Useful Features" of the
        maintenance guide.

 ** Windows(R) OS **

 You can check the System ROM date by a following procedure.

    1. Hold down <Windows> key and press <R> key.

    2. In the "Run" dialog box, type "msinfo32" and then click "OK".

    3. After "System Information" has started, select "System Summary".

    4. Check the System ROM version by the profile of "BIOS Version/Date".

 ** Linux(R) OS **

 You can check the System ROM date by a following procedure.

    1. Launch the terminal such as xterm.

    2. Execute the command as follows.

        # /usr/sbin/dmidecode | less

        Note: "#" means prompt. You do not need to input "#".

    3. Check the System ROM date by "BIOS Information->Release Date".

    Note: The dmidecode command has to be installed.

================================================================================
 Notes
================================================================================
  ** Notes in general **

  * Refer to "license_en.txt" about the user license agreement.

  * When you install the system ROM, the flashing mechanism writes over the
    backup ROM and saves current ROM as a backup, enabling you to switch easily
    to the alternate ROM version if the new ROM becomes corrupted for any
    reason. This feature protects the existing ROM version, even if you
    experience a power failure while flashing the ROM.

  * When Windows(R) BitLocker(TM) function is set to "Enabled", install the
    System ROM after making the function "Disabled". Then make the function
    "Enabled" after install and reboot of the system. If you install the system
    ROM without making the function "Disabled", you may need the recovery
    password when you boot the system.

  * This software does not support a virtualized environment such as hyper
    visor, guest OS, etc. Please install either on the OS which this software
    supports or with the method of offline installation.

  * To meet firmware dependencies, you can update iLO firmware by latest
    Starter Pack. And you can update Server Platform Services(SPS) firmware by
    latest "Server Platform Services(SPS) firmware update module".
    You can download latest update module(s) from the following web site.
    https://www.nec.com/express
    ("Support & Downloads" of the page top - PCs & Servers - Servers - Downloads
    - Select Model)

  ** Note for Windows(R) OS environment and Linux(R) OS environment **

  * This software will access to iLO5 (Baseboard Management Controller). It is
    required that the "iLO 5 Channel Interface Driver" (CHIF) must be installed.
    The CHIF driver can be installed by using EXPRESSBUILDER or "Starter Pack".

--------------------------------------------------------------------------------
[Revision history]
Version:3.72 (01/09/2026)

Upgrade Requirement: Recommended 
                     - Update to this version at your earliest convenience.

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - This version of the System ROM should be paired with Server Platform Services
   (SPS) Firmware 5.1.5.103 or later.

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Addressed an issue where the system iLO Remote Console could become 
   unresponsive when a warning message appeared in RBSU.

Version:3.70 (08/08/2025)

Upgrade Requirement: Recommended 
                     - Update to this version at your earliest convenience.

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - This version of the System ROM should be paired with Server Platform Services
   (SPS) Firmware 5.1.5.103 or later.

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Addressed following security vulnerabilities.
    CVE-2025-20064, CVE-2025-20027, CVE-2025-20028

 - Updated microcode for Processor.
     Intel(R) Xeon(R) E Processor
     Intel(R) Pentium(R) Gold Processor Series
     8th Generation Intel(R) Core(TM) i3 Processors

Version:3.60 (05/16/2025)

Upgrade Requirement: Recommended 
                     - Update to this version at your earliest convenience.

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - This version of the System ROM should be paired with Server Platform Services
   (SPS) Firmware 5.1.5.5 or later.

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Updated microcode for Processor. This version mitigates security 
   vulnerability of CVE-2024-45332.
     Intel(R) Xeon(R) E Processor
     Intel(R) Pentium(R) Gold Processor Series
     8th Generation Intel(R) Core(TM) i3 Processors

 - Removed Expired SUSE and Vmware Certificates.

 - Addressed an issue where the Name field of the Logical Drive under MR 
   controller page might be missing or changed unintentionally after exiting 
   and going back to the MR controller page.

Version:3.52 (02/21/2025)

Upgrade Requirement: Critical - Update to this version immediately.

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - This version of the System ROM should be paired with Server Platform Services
   (SPS) Firmware 5.1.5.5 or later.

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Updated microcode for Processor. This version mitigates security 
   vulnerability of  CVE-2024-28956, CVE-2024-36293.
     Intel(R) Xeon(R) E Processor
     Intel(R) Pentium(R) Gold Processor Series
     8th Generation Intel(R) Core(TM) i3 Processors

 - Added pop-up message for all Intelligent Provisioning boot paths to warn 
   users of the risk of data loss.

Version:3.50 (01/16/2025)

Upgrade Requirement: Recommended 
                     - Update to this version at your earliest convenience.

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - This version of the System ROM should be paired with Server Platform Services
   (SPS) Firmware 5.1.5.5 or later.

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Addressed an issue where the system would uses UUID for IPV6 DHCP even when 
   the IPv6 DHCP Unique Identifier option(*1) is set to DUID-LLT.
    (*1) System Configuration > BIOS/Platform Configuration(RBSU)
         > Network Options > Network Boot Options
         > IPv6 DHCP Unique Identifier

Version:3.40 (08/01/2024)

Upgrade Requirement: Recommended 
                     - Update to this version at your earliest convenience.

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - This version of the System ROM should be paired with Server Platform Services
   (SPS) Firmware 5.1.4.913.

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 - If the system ROM version is v3.40 (08/01/2024), you cannot enable or disable
   new boot devices, nor can you save these settings in the UEFI Boot Order 
   Control menu(*1).
    (*1) BIOS/Platform Configuration (RBSU) > Boot Options 
         > UEFI Boot Order Control.
   
 Enhancements and problem fixes:
 - Updated microcode for Intel(R) Xeon(R) Scalable Processor family.
   Addressed following security vulnerabilities.
    CVE-2024-24853
 
 - Addressed an issue where the "Physical Drive missing" message appears twice
   in POST when a drive was removed and rebooted with incorrect severity in IML.

 - Addressed an issue where pressing the <F12> key and selecting [Save and Exit]
   in the UEFI Boot Order menu unexpectedly clears the boot order.
         System Configuration > BIOS/Platform Configuration(RBSU)
         > Boot Options > UEFI Boot Settings > UEFI Boot Order

 - Addressed an issue where a RSoD might occur during the update of
   SAS drive firmware using Starter Pack. 

Version:3.10 (05/16/2024)

Upgrade Requirement: Recommended 
                     - Update to this version at your earliest convenience.

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - This version of the System ROM should be paired with Server Platform Services
   (SPS) Firmware 5.1.4.913.

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Addressed following security vulnerabilities.
    CVE-2023-45229, CVE-2022-36763, CVE-2022-36764, CVE-2021-38578, 
    CVE-2023-5678, CVE-2024-0727

 - Added a new C6 Without C1E State parameter to Minimum Processor Idle Power
   Core C-State Options.
          System Configuration > BIOS/Platform Configuration(RBSU) 
          > Power and Performance Options 
          > Minimum Processor Idle Power Core C-State

Version:3.00 (02/01/2024)

Upgrade Requirement: Recommended 
                     - Update to this version at your earliest convenience.

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - And, when system updated to System ROM v2.20 (10/27/2020) or later, it should
   be updated Server Platform Services(SPS) Firmware 5.1.4.208 or later
   at the same time.

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Addressed following security vulnerabilities.
    CVE-2023-45853, CVE-2021-38575, CVE-2023-45229, CVE-2023-45230,
    CVE-2023-45231, CVE-2023-45232, CVE-2023-45233, CVE-2023-45234,
    CVE-2023-45235, CVE-2023-45236, CVE-2023-45237

 - This version mitigates a security vulnerability (CVE-2023-3817) in OpenSSL.

 - Addressed an issue where the iSCSI SW IPv6 HDD could not be found under OS
   when iSCSI IP Address Type option is set to Auto in BIOS/Platform 
   Configuration (RBSU) iSCSI Attempt Configuration menu.
         System Configuration > BIOS/Platform Configuration(RBSU) 
         > Network Options > iSCSI Configuration > Add an iSCSI Attempt 
         > iSCSI Network Interface Selection > iSCSI Attempt Configuration

Version:2.90 (10/19/2023)

Upgrade Requirement: Recommended 
                     - Update to this version at your earliest convenience.

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - And, when system updated to System ROM v2.20 (10/27/2020) or later, it should
   be updated Server Platform Services(SPS) Firmware 5.1.4.208 or later
   at the same time.

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Replaced AC power with external power in the help text of Automatic Power-On
   option. 

 - Addressed an issue where system might hang while accessing IML log from RBSU.

Version:2.80 (07/20/2023)

Upgrade Requirement: Recommended 
                     - Update to this version at your earliest convenience.
                     
 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - And, when system updated to System ROM v2.20 (10/27/2020) or later, it should
   be updated Server Platform Services(SPS) Firmware 5.1.4.208 or later
   at the same time.

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Updated microcode for Processor.  This version mitigates security 
   vulnerability of CVE-2022-44611, CVE-2022-40982.
     Intel(R) Xeon(R) E Processor
     Intel(R) Pentium(R) Gold Processor Series
     8th Generation Intel(R) Core(TM) i3 Processors

 - This version mitigates a security vulnerability (CVE-2023-2650) in OpenSSL.

 - Addressed an issue where iLO embedded device health info would display blank 
   content under System Utilities when the Select Language option was set to 
   Japanese or Chinese.

Version:2.72 (04/20/2023)

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - And, when system updated to System ROM v2.20 (10/27/2020) or later, it should
   be updated Server Platform Services(SPS) Firmware 5.1.4.208 or later
   at the same time.

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Updated microcode for Processor.  This version mitigates security 
   vulnerability of CVE-2022-33894, CVE-2022-38087.
     Intel(R) Xeon(R) E Processor
     Intel(R) Pentium(R) Gold Processor Series
     8th Generation Intel(R) Core(TM) i3 Processors

 - Address an issue where an abnormal power-on-password dialog would pop up even
   though user did not set a Power On Password.

 - Addressed an issue where the TPM status between RBSU and iLO web interface 
   were not synchronized.

Version:2.68 (01/12/2023)

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - And, when system updated to System ROM v2.20 (10/27/2020) or later, it should
   be updated Server Platform Services(SPS) Firmware 5.1.4.208 or later
   at the same time.

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Addressed following security vulnerabilities.
    CVE-2022-26837, CVE-2022-33894

 - This version mitigates a security vulnerability (CVE-2022-37434)
   in zlib library.

 - Addressed an issue where some Chinese and Japanese translations were missing 
   from RBSU.

 - Addressed an issue that system will hang when BIOS tries to print a large IML
   message on POST screen.

 - Addressed an issue when system discovers thousands of LUNs and was trying to 
   create thousands of boot options for each LUN. System cannot add, delete or 
   adjust new boot options on iLO web and RBSU after rebooting. System becomes 
   unstable unless loading manufacture defaults.

Version:2.64 (10/13/2022)

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - And, when system updated to System ROM v2.20 (10/27/2020) or later, it should
   be updated Server Platform Services(SPS) Firmware 5.1.4.208 or later
   at the same time.

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Added support to show manufacturing date for DIMMs in SMBIOS.

 - Addressed an issue where firmware BootTimer would cause a black screen hang 
   when switching TPM 1.2 to 2.0.

Version:2.60 (07/14/2022)

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - And, when system updated to System ROM v2.20 (10/27/2020) or later, it should
   be updated Server Platform Services(SPS) Firmware 5.1.4.208 or later
   at the same time.

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - This version mitigates a security vulnerability (CVE-2022-0778,
   CVE-2022-1292, CVE-2022-2068) in OpenSSL.

 - This version mitigates a security vulnerability (CVE-2022-27404,
   CVE-2022-27405, CVE-2022-27406) in FreeType library.

 - This version mitigates a security vulnerability (CVE-2019-7317) 
   in libpng library.
 
 - Removed PCIe Bifurcation Options menu in RBSU.

Version:2.58 (04/14/2022)

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - And, when system updated to System ROM v2.20 (10/27/2020) or later, it should
   be updated Server Platform Services(SPS) Firmware 5.1.4.208 or later
   at the same time.

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Updated microcode for Processor. This version mitigates security
   vulnerability of INTEL-SA-00614, INTEL-SA-00617.
    Intel(R) Xeon(R) E Processor
    Intel(R) Pentium(R) Gold Processor Series
    8th Generation Intel(R) Core(TM) i3 Processors

 - Updated hardware initialization code. This version mitigates security
   vulnerability of INTEL-SA-00601.

 - This version mitigates a security vulnerability (CVE-2018-25032)
   in zlib library.

 - Addressed an issue where RAID controller names were not displayed correctly
   in the PCIe Device Configuration menu in RBSU or the One-Time Boot menu
   when the Select Language option in System Utilities was set to non-English.
         System Configuration > BIOS/Platform Configuration (RBSU)
         > PCIe Device Configuration

Version:2.56 (01/20/2022)

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - And, when system updated to System ROM v2.20 (10/27/2020) or later, it should
   be updated Server Platform Services(SPS) Firmware 5.1.4.208 or later
   at the same time.

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Addressed following security vulnerabilities.
    CVE-2021-0092, CVE-2021-0127, CVE-2021-0156, CVE-2021-0157

 - Addressed an issue where Boot Mode option setting changed after
   EXPRESSBUILDER flash complete and system may hang when entring
   EXPRESSBUILDER after changed Boot Mode option setting.

 - Remove IPMI Watchdog Timer support from RBSU.

Version:2.54 (10/21/2021)

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - And, when system updated to System ROM v2.20 (10/27/2020) or later, it should
   be updated Server Platform Services(SPS) Firmware 5.1.4.208 or later
   at the same time.

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Updated microcode for Processor. This version mitigates security
   vulnerability of INTEL-SA-0562 for CVE-2021-0157.
    Intel(R) Xeon(R) E Processor
    Intel(R) Pentium(R) Gold Processor Series
    8th Generation Intel(R) Core(TM) i3 Processors

Version:2.52 (09/16/2021)

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - And, when system updated to System ROM v2.20 (10/27/2020) or later, it should
   be updated Server Platform Services(SPS) Firmware 5.1.4.208 or later
   at the same time.

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Addressed an issue where High Precision Event Timer was not showing up
   in Windows(R) Device Manager.

Version:2.50 (07/20/2021)

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - And, when system updated to System ROM v2.20 (10/27/2020) or later, it should
   be updated Server Platform Services(SPS) Firmware 5.1.4.208 or later
   at the same time.

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Addressed following security vulnerabilities.
    CVE-2019-14584, CVE-2021-28211, CVE-2021-28210.

 - Addressed an issue where a PCIe option card or an unattached NVMe M.2 device
   may not show up correctly in Device Inventory or storage page in iLO Web
   Interface.

Version:2.32 (06/10/2021)

 Notes:
 - When PCI option card is not installed in PCI slot 1, update this System ROM.
   The name of PCI option card attached on PCI Slot 1 is indicated as
   "Empty Slot 1" on the iLO web interface, and if an error was detected
   in PCI Slot 1, the error will not be recorded correctly in IML when meets
   all the following conditions.
    - System ROM version: v2.32 (06/10/2021)
    - iLO5 Firmware version: 2.40 or later

 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - And, when system updated to System ROM v2.20 (10/27/2020) or later, it should
   be updated Server Platform Services(SPS) Firmware 5.1.4.208 or later
   at the same time.

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 - When updated to System ROM v2.32 (06/10/2021), NVMe which was not installed
   will be displayed as the following, but cannot be used.
    - Firmware & OS Software - Firmware: NVMe Drive
    - System Information - Storage: NVMe SSD
    - System Information - Device Inventory: PCI-E Slot 1

 Enhancements and problem fixes:
 - Addressed an issue where systems running System ROM 2.20 or later and
   configured with an Intel Xeon E-2224 CPU and Hynix 16G DDR4 DIMM may
   occasionally encounter the following error message in the Integrated
   Management Log (IML).
    - Code: 0x221 Unknown Initialization Error...
   The manufacturer of the DIMM can be checked from iLO web interface
   by following the steps below.
    1. Select "System Information tab" from the right menu.
    2. Select "Memory" from the left menu.
    3. Select DIMM to check from "Physical Memory".
    4. Check "Vendor" from "Memory Details" displayed from the right menu.

Version:v2.30 (05/24/2021)

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - And, when system updated to System ROM v2.20 (10/27/2020) or later, it should
   be updated Server Platform Services(SPS) Firmware 5.1.4.208 or later
   at the same time.

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Added a new IPMI Watchdog Timer option to Server Availability menu. 
    System Configuration > BIOS/Platform Configuration (RBSU)  > System Options
    > Server Availability

 - Added a new UEFI Variable Access Firmware option to Server Security menu.
   System Configuration > BIOS/Platform Configuration (RBSU)  > Server Security
 
 - Updated microcode for Processor. This version mitigates security
   vulnerability of INTEL-SA-00464.
    Intel(R) Xeon(R) E Processor
    Intel(R) Pentium(R) Gold Processor Series
    8th Generation Intel(R) Core(TM) i3 Processors

 - Updated hardware initialization code. This version mitigates security
   vulnerability of INTEL-SA-00463.

 - Addressed an extremely rare issue where the Real Time Clock may become
   corrupted and an unexpected change on a server boot.

 - Addressed an issue where the server system fans may run higher than
   anticipated when a server is configured with SATA HDD/SSD (N8150-596,
   N8150-545, N8150-1734, etc.).

Version:2.20 (10/27/2020)

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - And, when system updated to System ROM v2.20 (10/27/2020) or later, it should
   be updated Server Platform Services(SPS) Firmware 5.1.4.208 or later
   at the same time.

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Added a new BIOS/Platform Configuration (RBSU) option to Memory Options
   called Refresh Watermarks. When selecting the Low Watermark setting,
   the memory controller will help reduce susceptibility to a DDR4 RowHammer
   attack. It is expected that a memory performance impact will be seen when
   enabling the Low Watermark setting.
    System Utilities > System Configuration > RBSU > Memory Options

 - Updated the RESTful API BIOS Attribute Registry resources to match the
   latest BIOS/Platform Configuration(RBSU) options.

 - Updated microcode for Processor. 
    Intel(R) Xeon(R) E Processor
    Intel(R) Pentium(R) Gold Processor Series
    8th Generation Intel(R) Core(TM) i3 Processors

 - Addressed following security vulnerabilities.
    INTEL-SA-00381, INTEL-SA-00389, INTEL-SA-00358.

 - Addressed an issue where system may suddenly stop responding, shutdown or
   restart unexpectedly.
   Integrated Management Log (IML) contains the following information.
    - Class: 0x32, Code: 0x389 Unexpected Shutdown and Restart...
   And, it should be updated Server Platform Services(SPS) Firmware
   at the same time.
   For the detail of the SPS firmware, refer to "Notes" in [About the software].

Version:2.18 (06/24/2020)

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Updated microcode for Processor. This version mitigates security
   vulnerability of CVE-2020-0543, CVE-2020-0548, CVE-2020-0549.
    Intel(R) Xeon(R) E Processor
    Intel(R) Pentium(R) Gold Processor Series
    8th Generation Intel(R) Core(TM) i3 Processors

Version:2.16 (05/25/2020)

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:

 - Updated to the latest thermal support for the platform.

 - Updated the RESTful API BIOS Attribute Registry resources to match the
   latest BIOS/Platform Configuration(RBSU) options.

 - Updated microcode for Processor.
    Intel(R) Xeon(R) E Processor
    Intel(R) Pentium(R) Gold Processor Series
    8th Generation Intel(R) Core(TM) i3 Processors.
 
 - Addressed following security vulnerabilities.
    CVE-2020-0528, CVE-2020-0529

 - Addressed an issue where the serial port would not function properly when
   the Serial CLI Status was also enabled on the server. This could lead to 
   the serial BAUD rate not being configured properly and the serial output from
   the host would be corrupted or no output would be seen.
         System Configuration > BMC Configuration Utility > Setting Options
         > Serial CLI Status

 - Addressed an extremely rare issue where the server could become unresponsive
   in POST when configured in Legacy BIOS Mode at Boot Mode option when a
   USB Mouse is attached. This issue does not impact systems configured in
   UEFI Mode.
         System Configuration >  RBSU > Boot Options > Boot Mode

 - Addressed an issue where boot devices could disappear from the Boot Options
   menu when pressing the <F10> or <F12> key to save boot order changes.
         System Configuration >  RBSU > Boot Options

 - Addressed an issue where the server may become unresponsive during POST when
   both iLO and the server are reset simultaneously.

 - Addressed an issue where the System Utilities System Information data could
   not be successfully exported to an FTP network location. 

Version:2.14 (03/09/2020)

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Updated the UEFI driver of Smart Array S100i Software RAID.
   Addressed an issue where the Smart Array S100i Software RAID may experience
   potential data inconsistency during initial configuration or operation of
   a RAID volume configured in RAID 0/1/10.

Version:2.12 (12/06/2019)

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Updated microcode for Processor. This version mitigates security
   vulnerability of CVE-2019-11157.
    Intel(R) Xeon(R) E Processor
    Intel(R) Pentium(R) Gold Processor Series
    8th Generation Intel(R) Core(TM) i3 Processors

Version:2.10 (09/12/2019)

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 - Improved the function to set the memory frequency. Fault tolerance of
   the system is improved.
   The memory frequency will be set 2666MHz when all of the following
   requirements are met. If not satisfied, the memory frequency will be set
   2400MHz.
    - Intel (R) Xeon (R) E Processor is equipped.
    - Memories with the same part number are mounted on the same channel.
   
   Note) The memory part number can be confirmed in the following items of
         System Utilities.
          System Utilities > System Information > Memory Information >
          Part Number

   Note) In case of R110j-1, memory frequency will be set lower frequency
         depending on memory configuration.

 Enhancements and problem fixes:
 - Addressed following security vulnerabilities.
    CVE-2017-5715, CVE-2018-12126, CVE-2018-12127, CVE-2018-12130, 
    CVE-2019-11135, CVE-2018-11091

 - Updated microcode for processor. 
    Intel(R) Xeon(R) E Processor
    Intel(R) Pentium(R) Gold Processor Series
    8th Generation Intel(R) Core(TM) i3 Processors

Version:2.00 (09/05/2019)

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 Enhancements and problem fixes:
 - Updated to the latest thermal support for the platform.

 - Addressed following security vulnerabilities.
    CVE-2019-1559

 - Addressed an issue where the Intel Software Guard Extensions(SGX) Remote
   attestation functionality may not work properly.

 - Addressed an issue where the Server Backup and Restore functionality may not
   work properly if initiated through the RESTful API returning a message "An
   internal error occurred during RIS operation".

 - Addressed an issue where the system would not boot to a USB drive when
   a non-bootable (non-formatted) drive was also present in the system.
   This issue only impacts systems configured in Legacy BIOS Mode.
    System Utilities > System Configuration >
    RBSU > Boot Options > Boot Mode

Version:1.22 (04/04/2019)

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 Enhancements and problem fixes:
 - Updated microcode for processor. This version mitigates security
   vulnerability of CVE-2018-12126, CVE-2018-12130, CVE-2018-12127, 
   CVE-2019-11091.
    Intel(R) Xeon(R) E Processor
    Intel(R) Pentium(R) Gold Processor Series
    8th Generation Intel(R) Core(TM) i3 Processors

Version:1.20 (02/02/2019)

 Notes:
 - Do not update if Intel(R) Software Guard Extensions(SGX) is set to Enabled 
   in a system equipped with the following specific processors. The factory
   default setting is "Disabled".

    System Utilities > System Configuration >
    RBSU > Processor Options >  
    Intel(R) Software Guard Extensions(SGX)

   Note) CPU board(4C/i3-8300) [N8101-1515]
         CPU board(2C/Pentium G5400) [N8101-1512]

 Enhancements and problem fixes:
 - Added a new "Backup and Restore Settings" menu to "System Default Options" 
   in the BIOS/Platform Configuration (RBSU). This option allows you to save 
   the BIOS configuration to a USB storage device. 

 - Updated description of Japanese and Chinese for System Utilities.

 - Updated the RESTful API BIOS Attribute Registry resources to match the 
   latest BIOS/Platform Configuration(RBSU) options.

 - Addressed following security vulnerabilities.
    CVE-2018-3613, CVE-2017-5731, CVE-2017-5732, CVE-2017-5733, CVE-2017-5734,
    CVE-2017-5735, CVE-2018-3630, CVE-2018-12178, CVE-2018-12179, 
    CVE-2018-12180, CVE-2018-12181, CVE-2018-12182, CVE-2018-12183

 - Addressed an issue where certain PCIe option cards may not train properly 
   and cause the system to hang during POST.

 - Addressed an issue where iLO virtual media may not boot properly after 
   setting the "Boot on Next Reset" option in the "Remote Console and Media - 
   Virtual Media" settings in the iLO web interface.

 - Addressed an issue where the AHS Download application from the Embedded 
   Applications in System Utilities may fail to work properly with iLO 
   firmware 1.30 or later.

 - Addressed an issue where an optional SATA DVD drive may not unlock and 
   allow media to be ejected after an operating system reboot.

 - Addressed an issue where the system may become unresponsive during boot and 
   experience a Red Screen (RSOD) when booting in Legacy BIOS Mode with a 
   M.2 SATA SSD installed. This issue does not impact systems in UEFI Mode.

--------------------------------------------------------------------------------
[Copyright and Trademark]

All contents on this software are the copyright of NEC Corporation or the
third-party software developer. All other contents mentioned herein are
copyright of their respective owners.

Microsoft, Windows, Windows Server are trademarks or registered trademarks of
Microsoft Corporation in the United States and other countries.
Linux(R) is a registered trademark of Linus Torvalds in the United States and
other countries.
Red Hat is a trademark or a registered trademark of Red Hat Inc. in the United
States and other countries.

All other company names and product names mentioned herein are registered
trademarks or trademarks of their respective owners.

--------------------------------------------------------------------------------
   Copyright NEC Corporation 2026
